# Getting started tasks

This section describes how to perform the following steps:

Step | Action | For more information, refer to...
1 | Configure the CG board and boot the board as a Fusion board using oamsys. | Configuring CG boards, Customizing the board configuration, or the board's hardware documentation.
2 | Run the msppxsr demonstration program to test the MSPP API and CG board DSP resources by creating MSPP endpoints, channels, and connections. Running msppxsr requires two Fusion systems connected to the same network and a device for generating calls at both ends. | MSPP exerciser: msppxsr.
3 | Run CG board utilities to set up the Ethernet interface and gather statistics about transferred data. | Using CG board utilities or the appropriate CG board manual.
4 | Run the msppsamp demonstration program to transfer data between two Fusion systems. | Fusion nailed-up sample: msppsamp.