# NMS_V5ResetE1Status

Resets status information for a specified E1 link.

#### Prototype

NMS_V5_RESULT_T NMS_V5ResetE1Status ( NMS_V5_INTERFACE_ID_T interfaceId NMS_V5_CHANNEL_LOCATION_T *e1_loc)

Argument | Description
interfaceId | Interface ID of a provisioned interface.
e1_loc | Pointer to the E1 link location for which to reset status information. typedef union _NMS_V5_E1_LOCATION_T { struct { DWORD boardNb; DWORD trunkNb; } CG; }NMS_V5_E1_LOCATION_T See the Details section for field descriptions.

#### Return values

Return value | Description
NMSV5_SUCCESS |
NMSV5_INTERNAL_FAILURE | Internal failure. Refer to the trace log for more information.
NMSV5_INVALID_E1 | Specified E1 link is not provisioned on this interface.
NMSV5_INVALID_INTERFACE_ID | Specified interface is not provisioned.
NMSV5_NOT_INITIALIZED | NMS V5 library was not initialized with NMS_V5Initialize.

#### Details

NMS_V5ResetE1Status resets status information for a specified E1 link. Applications can only reset status information for E1 links provisioned on the active variant of an interface. The NMS_V5_E1_LOCATION_T structure includes the following values:

Field | Description
boardNb | Logical board number where the E1 link is located (as defined by NMS OAM).
trunkNb | Logical trunk number associated with the E1 link (as defined by NMS OAM).

#### See also

NMS_V5GetE1Status

#### Example

void ResetE1Status( void )
{
NMS_V5_RESULT_T NmsResult;
DWORD InterfaceId;
NMS_V5_E1_LOCATION_T E1Location;
printf("NMS_V5ResetE1Status:\n");
/* Get parameters */
promptdw_nodft("Enter InterfaceId", &InterfaceId);
printf("Enter E1 location:\n");
GetE1LocationNMS( &E1Location );
NmsResult = NMS_V5ResetE1Status( InterfaceId, E1Location );
printf ("NMS_V5ResetE1Status:
Result=%s\n",PRINT_RESULT(NmsResult));
}