# acu_ss_notify_transfer_ret_result

Indicates that a notify transfer operation was successful.

#### Variant

ETS 300/Q.SIG

#### Operation ID

ACU_OP_ID_NOTIFY_TRANSFER

#### OpType

ACU_OP_TYPE_RETRES

#### Structure

struct acu_ss_notify_transfer_ret_result
{
struct acu_ext_hdr ext_hdr; /* Extension header */
struct acu_ss_hdr ss_hdr; /* Supp. services header */
struct acu_party_name redir_name; /* Provides name of redirecting party*/
struct acu_party_num redir_nb; /* Provides no. of redirecting party */
struct acu_party_subaddress redir_sub; /* Provides subaddress of */
}; /* redirecting party */

#### Fields

Field | Description | Mandatory in messages from ETS 300 user-side app? | Mandatory in messages from Q.SIG PINX serving user B or C? | Mandatory in messages to Q.SIG PINX serving user A and (B or C)?
--- | --- | --- | --- | ---
redir_name | Indicates supplementary service is invoked and remaining name fields are valid. For Q.SIG only. | Yes | Optional | Not included
redir_nb | Indicates number of joined party. | Not included | Optional | Optional
redir_sub | Indicates subaddress of joined party. If response_rq is on in the invocation request, the application should send this information back. | Not included | Optional | Optional