# acu_ss_notify_diversion_ret_result

Indicates that a notify diversion operation was successful.

#### Variant

ETS 300/Q.SIG

#### Operation ID

ACU_OP_ID_NOTIFY_DIVERSION

#### OpType

ACU_OP_TYPE_RETRES

#### Structure

struct acu_ss_notify_diversion_ret_result
{
struct acu_ext_hdr ext_hdr; /* Extension header */
struct acu_ss_hdr ss_hdr; /* Supp. services header */
struct acu_party_name redir_name; /* Redirection name */
ushort pres_allowed; /* Indicates whether diverted-to */
pad6 /* number can be presented(ON/OFF)*/
};

#### Fields

Field | Description | Mandatory in messages to originating Q.SIG node's app? | Mandatory in messages from diverted-to user Q.SIG node's app?
--- | --- | --- | ---
redir_name | The name of the diverted-to user. | Optional | Optional
pres_allowed | (ON/OFF) Indicates whether the diverted-to user allows presentation of number and name. | Yes | Yes