# acu_ss_enquire_divert_ret_result

Indicates that an enquire diversion invocation request was successful.

#### Variant

ETS 300

#### Operation ID

ACU_OP_ID_ENQUIRE_DIVERSION

#### OpType

ACU_OP_TYPE_RETRES

#### Structure

struct acu_ss_enquire_divert_ret_result
{
struct acu_ext_hdr ext_hdr; /* Extension header */
struct acu_ss_hdr ss_hdr; /* Supp. services header */
struct op_byte_field remote_enabled;/*ON/OFF indicates remotely enabled */
struct op_byte_field procedure; /* From ACU_SS_DIVERSION_ constants */
struct op_byte_field basic_service; /* From ACU_SS_BASIC_SERVICE_ constants */
struct acu_address diverted_to; /* Address that served user is */
/* forwarded to */
struct acu_party_num served_user; /* Served user's address */
uchar complete; /* ON when no more messages */
/* coming, OFF if more coming */
/* Note: when ON, other fields */
pad7 /* might not be invoked */
};

#### Fields

Field | Description | Mandatory in messages from ETS 300 user-side app?
--- | --- | ---
remote_enabled | ON/OFF, indicates remotely enabled. | Not included
procedure | CFU, CFB, CFNR. From AU_SS_DIVERSION constants. | Optional
basic_service | Voice and data. From AU_SS_BASIC_SERVICE constants. If absent, applies to all services. | Optional
diverted_to | Number that the served user is forwarded to. If absent, applies to all served users. | Optional
served_user | Served users address. | Optional
complete | ON when no more messages are coming. OFF if more are coming. Note: When ON, other fields might not be invoked. | Yes