# acu_ss_aoc_request_ret_result

Indicates that an advice of charge service request was successful.

#### Variant

ETS 300

#### Operation ID

ACU_OP_ID_AOC_REQUEST

#### OpType

ACU_OP_TYPE_INVOKE

#### Structure

struct acu_ss_aoc_request_ret_result
{
struct acu_ext_hdr ext_hdr; /* Extension header */
struct acu_ss_hdr ss_hdr; /* Supp. services header */
uchar aoc_s; /* AOC-S services active (ON/OFF)*/
uchar aoc_d; /* AOC-D services active (ON/OFF)*/
uchar aoc_e; /* AOC-E services active (ON/OFF)*/
pad5
};

#### Fields

Field | Description | Mandatory in messages to ETS 300 user-side application?
--- | --- | ---
aoc_s | (ON/OFF) AOC-S services active/inactive. | Yes
aoc_d | (ON/OFF) AOC-D services active/inactive. | Yes
aoc_e | (ON/OFF) AOC-E services active/inactive. | Yes