# acu_ss_deact_divert_invoke

Requests deactivation of call diversion services for a user.

#### Variant

ETS 300

#### Operation ID

ACU_OP_ID_DEACTIVATE_DIVERSION

#### OpType

ACU_OP_TYPE_INVOKE

#### Structure

struct acu_ss_deact_divert_invoke
{
struct acu_ext_hdr ext_hdr; /* Extension header */
struct acu_ss_hdr ss_hdr; /* Supplementary serv. header */
struct acu_party_num served_user; /* User to deactivate diversion for*/
struct acu_party_num deactivating_user; /* User initiating the */
/* deactivation */
uchar procedure; /* From ACU_SS_DIVERSION_ constants*/
uchar basic_service; /* From ACU_SS_BASIC_SERVICE_ */
pad6 /* constants */
};

#### Fields

Field | Description | Mandatory in messages from ETS 300 user-side app?
--- | --- | ---
served_user | User to deactivate diversion for. | Optional
deactivating_user | User initiating the deactivation. | Not included
procedure | CFU/CFB/CFNR. From AU_SS_DIVERSION constants. | Yes
basic_service | Voice and data. From AU_SS_BASIC_SERVICE constants. If a basic service other than ACU_SS_BASIC_SERVICE_ALL_SERVICES is specified, call diversion is deactivated just for calls of that service type. | Yes