# T38UDP endpoint address structure

When the endpoint type is MSP_ENDPOINT_T38FDX, the application provides the following endpoint address information:

typedef struct tag_T38UDP_ENDPOINT_ADDR
{
// UDP parameters
char DestIpAddress[20];
WORD nDestPort;
char SourceIpAddress[20];
WORD nSourcePort;
} T38UDP_ENDPOINT_ADDR;

## T38UDP_ENDPOINT_ADDR

#### Dependent function: mspCreateEndpoint

Field | Type | Default | Units | Description
pDestIpAddress[20] | char | N/A | N/A | Destination IPv4 address in dot notation.
nDestPort | WORD | N/A | N/A | Destination UDP port number.
pSourceIpAddress[20] | char | N/A | N/A | Source IPv4 address in dot notation.
nSourcePort | WORD | N/A | N/A | Source UDP port number.