# NCCEVN_CALL_CONNECTED

Both parties are now connected.

#### State transition

To connected state from answering, placing, or proceeding call states.

#### Associated function

Unsolicited

#### Fields

Field | Description
callhd | Call handle.
value | Indicates the reason why the call was connected.

#### Reason codes

Reason code | Description
NCC_CON_ANSWERED | Call answered by nccAnswerCall.
NCC_CON_CED | Outbound CED detected.
NCC_CON_DIALTONE_DETECTED | Outbound CP dialtone (may be disabled).
NCC_CON_PROCEEDING | Do not run call progress.
NCC_CON_RING_BEGIN | Outbound ring detected.
NCC_CON_RING_QUIT | Outbound ring stop (soft speaker).
NCC_CON_SIGNAL | Connect by out-of-band signal.
NCC_CON_SIT_DETECTED | Outbound SIT detected.
NCC_CON_TIMEOUT | Outbound timeout.
NCC_CON_VOICE_BEGIN | Outbound voice detected.
NCC_CON_VOICE_END | Outbound voice ended.
NCC_CON_VOICE_EXTENDED | Outbound voice extended.
NCC_CON_VOICE_LONG | Outbound voice long.
NCC_CON_VOICE_MEDIUM | Outbound voice medium.

#### Details

NCCEVN_CALL_CONNECTED indicates that a call reached the connected state. The event value field contains the reason for the connection.