# Running nccxfer

nccxfer demonstrates rerouting an incoming call.

#### Usage

nccxfer [options]

where options are:

Option | Description
--- | ---
-A xxxmgr | Specifies the NaturalAccess manager to use for the ADI API. Default is ADIMGR.
-b n | Specifies the board number n. Default is 0.
-s n:m | Specifies the MVIP stream and timeslot for the first channel. Default is 0:0.
-p protocol | Specifies the protocol to run. Default is lps0.
-i n | Specifies the number of call iterations (0=infinite).
-m n | Specifies the method of transfer. Valid values for n:
Value | Description
1 | Transfer on PROCEEDING (after dial) (default)
2 | Transfer on ALERTING (ringing)
3 | Transfer on CONNECTED (first voice or signal)
4 | Manual (call screening)

#### Featured functions

nccAutomaticTransfer, nccTransferCall

#### Description

Party A calls party B (which is the demonstration program) and requests a transfer to party C. nccxfer (party B) then calls party C. It reports success or failure at one of several stages, depending on the selected transfer method. If -m 4 is specified on the command line, nccxfer asks party C whether it should complete the transfer, or report failure.

#### Procedure

Begin with three telephone lines: two (A and C) with two 2500-type telephone sets, and one (B) connected to the board. Lines B and C must be connected to a common PBX.

Complete the following steps to run nccxfer:

Step | Action
1 | Specify the proper board and MVIP stream, and start the configuration utility.
2 | Start nccxfer by entering the following at the prompt: nccxfer [ -b n -s n:m -p protocol -i n -m n ] Make sure to specify a transfer method.
3 | From line A, call line B. The demonstration answers.
4 | When the program requests an extension to try, dial the extension of line C. The demonstration calls line C.
5 | Answer line C.

With transfer method 4, the demonstration offers you a chance to refuse the call. The other transfer modes report success or failure at earlier stages, sometimes before the transfer is actually completed.