# Outbound call events

Event | Informational/ Transitional | Solicited/ Unsolicited | Indicates that...
--- | --- | --- | ---
NCCEVN_CALL_CONNECTED | Transitional | Unsolicited | Both parties are connected.
NCCEVN_CALL_PROCEEDING | Transitional | Unsolicited | The switch accepted the call setup. The receiving side is being rung.
NCCEVN_PLACING_CALL | Transitional | Solicited | A call was placed successfully.
NCCEVN_REMOTE_ALERTING | Informational | Solicited | The remote end is ringing.
NCCEVN_REMOTE_ANSWERED | Informational | Solicited | The remote end is answering the call.