# NCCEVN_REMOTE_ANSWERED

The remote end is answering the call.

#### State transition

None.

#### Associated function

nccPlaceCall

#### Fields

Field | Description
callhd | Call handle.
value | Reason this event took place.

#### Reason codes

Reason code | Description
NCC_ANSWER_MODEM | Due to modem detection.
NCC_ANSWER_SIGNAL | Due to out-of-band signaling.
NCC_ANSWER_VOICE | Due to voice detection.

#### Details

NCCEVN_REMOTE_ANSWERED is generated at the first positive indication that the remote party has answered (out-of-band signaling, voice, or modem tone). The event value field contains the indication type.

This event is generated only if the NCC_REPORT_ANSWERED bit is set in the NCC.START.eventmask parameter (see NCC API global parameters).