# Default connections for a standalone board

For a standalone CX 2000 board, disable H.100 connectivity in the configuration file (Clocking.HBus.ClockMode = DISABLE). In this case, default connections are made on the board to connect voice and signaling information to DSP resources.

Station type | Setting
--- | ---
Full duplex voice station | Local:0:0..47 => Local:5:0..47, Local:4:0..47 => Local:1:0..47 for 48 ports Local:0:0..31 => Local:5:0..31, Local:4:0..31 => Local:1:0..31 for 32 ports
Full duplex signaling station | Local:2:0..47 => Local:7:0..47, Local:6:0..47 => Local:3:0..47 for 48 ports Local:2:0..31 => Local:7:0..31, Local:6:0..31 => Local:3:0..31 for 32 ports