# DSPStream.SignalIdleCode[x]

Sets the idle code for timeslots
on DSP signaling streams.

#### Syntax

DSPStream.SignalIdleCode[x] = signal_idlecode

x = 0-(n-1) (0-based trunk number or range of trunk numbers where n equals the number of trunks on the board.)

#### Access

Read/Write

#### Type

Integer

#### Default

0x0D

#### Allowed values

0x0000 - 0xFF

#### Example

DSPStream.SignalIdleCode[0..7] = 0x00

#### Details

The CG 6565C board signaling DSP uses this value to generate the idle pattern on the outbound signaling trunk.

All trunks must be configured with the same DSPStream.SignalIdleCode setting.

#### See also

DSPStream.SlotCount, DSPStream.VoiceIdleCode[x]