_j
0x 1 2
0x00 1 2 3
0x04 1 2 3
0x08 1 2 3
0x7500
0x7f
0xd
0xd5
0xff 1 2
0xffff
0xfh
11h
11k
12v
14x
1500vrms
1544m
2000c
2048m
20k
2mb
2mhz
2v9
3rd
49h
4lse
5aa5
5th
5v
5x 1 2
6060c
64k
6565c
6565e
66mhz
6khz
76go
8k 1 2
8lse
8mhz
a_clock 1 2 3 4
a2
a2auslsc
a2canls6
a2canls9
a2canlsn
a2eurlsc 1 2
a2jpnls6
a2jpnls9
a2jpnlsn
a2lpspi
a2usa
a2usadd6 1 2 3
a2usadd9 1 2
a2usals6 1 2 3
a2usals9 1 2
a2usalsn 1 2
a2usasl6 1 2 3
a2usasl9 1 2
aaaah
able
abort
above 1 2
ac 1 2 3 4
aca
accept 1 2
access 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65
accessed
accessing
accordance 1 2
according 1 2 3 4 5
accordingly 1 2 3
accuracy
achieve
acknowledgement
across 1 2
act 1 2
action 1 2 3 4 5 6 7
active 1 2
actively
activity
acts 1 2
actual
adapt 1 2
adaptation
adapted
adapter 1 2 3 4 5 6
adapts
add 1 2 3 4
added 1 2 3
adding
addition 1 2 3
additional 1 2 3 4 5 6 7 8 9
address 1 2 3 4
addresses
adequate
adhere
adi 1 2 3 4 5 6 7
adi_encode_alaw 1 2
adi_encode_g726 1 2
adi_encode_gsm
adi_encode_ima_24
adi_encode_ima_32
adi_encode_mulaw 1 2
adi_encode_nms_16 1 2
adi_encode_nms_24 1 2
adi_encode_nms_32 1 2
adi_encode_nms_64 1 2
adi_encode_oki_24
adi_encode_oki_32
adi_encode_pcm11m16 1 2
adi_encode_pcm11m8
adi_encode_pcm8m16 1 2
adicommandrecord
adievn_answering_call
adievn_call_connected
adievn_incoming_call
adievn_play_done
adievn_record_buffer_full
adievn_record_done
adievn_startprotocol_done
adirecordasync
adistartcallprogress
adistartdial
adistartdtmf
adistartdtmfdetector
adistartenergydetector
adistartmfdetector
adistartplaying
adistartprotocol
adistartreceivingfsk
adistartrecording 1 2
adistartsendingfsk
adistartsignaldetector
adistarttonedetector 1 2
adistarttones
adisubmitrecordbuffer
adjacent
adjust
adjustments
administration
adpcm 1 2
adsi 1 2
adsir 1 2
adsix 1 2

>>