# NCC.X.ADI_PLACECALL

The following table describes NCC.X.ADI_PLACECALL parameters:

NCC.X.ADI_PLACECALL
Dependent functions: nccPlaceCall, nccAutomaticTransfer
Field | Type | Default | Units | Description
--- | --- | --- | --- | ---
connectmask | DWORD | 0x0103 | mask | Controls which network events cause an outgoing call to transition to the connected state. A value can be formed by using the OR operator with any of the following bit masks: NCC_CON_ON_CED (0x0100): Modem detected NCC_CON_ON_DIALTONE (0x0200): Dial tone NCC_CON_ON_PROCEEDING (0x8000): Connect immediately NCC_CON_ON_RING_BEGIN (0x0800): Connect immediately NCC_CON_ON_SIGNAL (0x0001): Out-of-band signal NCC_CON_ON_SIT (0x0400): SIT detected NCC_CON_ON_VOICE_BEGIN (0x0002): Voice detected NCC_CON_ON_VOICE_END (0x0020): Voice ended NCC_CON_ON_VOICE_EXTENDED (0x0010): Extended voice NCC_CON_ON_VOICE_LONG (0x0008): Long voice NCC_CON_ON_VOICE_MEDIUM (0x0004): Medium length voice NCC_CON_RING_QUIT (0x0080): Ring ended
disconnectmask | DWORD | 0x0040 | mask | Controls which network events cause an outgoing call to disconnect (not complete). A value can be formed by using the OR operator with any of the following bit masks: NCC_DIS_ON_CED (0x0100): Dial tone NCC_DIS_ON_RING_BEGIN (0x0800): Call progress ring begin NCC_DIS_ON_RING_QUIT (0x0080): Call progress ring quit NCC_DIS_ON_TIMEOUT (0x0040): Call progress timeout NCC_DIS_ON_VOICE_BEGIN (0x0002): Voice detected NCC_DIS_ON_VOICE_END (0x0020): Voice ended NCC_DIS_ON_VOICE_EXTENDED (0x0010): Extended voice NCC_DIS_ON_VOICE_LONG (0x0008): Long voice NCC_DIS_ON_VOICE_MEDIUM (0x0004): Medium length voice