# ACU_PROGRESS_RQ

This topic describes:

- ACU_PROGRESS_RQ protocol variants

- ACU_PROGRESS_RQ macro descriptions and Q.931 IE

#### Purpose

Indicates progress request.

#### Conn_id

An allocated call.

## ACU_PROGRESS_RQ protocol variants

The following table lists the variants under which each macro is supported for this primitive. In this table, x indicates both NT and TE sides.

Macro | 4 E S S | E 1 0 | N I 2 | D M S | E T S I | V N 6 | H K G | A U S T E L 1 | N T T | K O R E A | T A I W A N | Q S I G | D P N S S | T 1 6 0 7
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acu_progress_rq_a_tsp_ie_list, Acu_progress_rq_tsp_ie_list_size | x | x | x | x | x | x | x | x | x | x | x | x | x | x
Acu_progress_rq_cause | x | x | x | x | x | x | x | x | x | x | x | x |  | x
Acu_progress_rq_cause_location | x | x | x | x | x | x | x | x | x | x | x | x |  | x
Acu_progress_rq_progress_description | x | x | x | x | x | x | x | x | x | x | x | x |  | x
Acu_progress_rq_progress_location | x | x | x | x | x | x | x | x | x | x | x | x |  | x

## ACU_PROGRESS_RQ macro descriptions and Q.931 IE

Macro | Description | Q.931 IE
--- | --- | ---
Acu_progress_rq_a_tsp_ie_list, Acu_progress_rq_tsp_ie_list_size | Pointer to (and size of) transparent IE buffer. | Does not map to an IE.
Acu_progress_rq_cause | Cause value. | Cause
Acu_progress_rq_cause_location | Cause location. | Cause
Acu_progress_rq_progress_description | Description for information element 0. See Progress description values for a list of valid values. | Progress indicator
Acu_progress_rq_progress_location | Location of information element 0. See Location values for a list of valid values and default setting information. | Progress indicator