<<

adapt 1 2 3 4 5
adaptation 1 2 3 4 5
adaptive
adapttime 1 2 3 4
add 1 2 3 4 5 6
added 1 2 3
addition 1 2 3 4
additional 1 2 3 4 5 6 7 8
addressed 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23
addresses 1 2 3 4
addrstruct
adequate
adi 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81
adi_
adi_a_bit 1 2 3 4
adi_ag_driver_only 1 2 3 4 5 6
adi_b_bit 1 2 3 4
adi_bit
adi_bit_
adi_board_info
adi_boardtype_ag2000
adi_boardtype_ag2000bri
adi_boardtype_ag2000c
adi_boardtype_cg6060
adi_boardtype_cg6060c
adi_boardtype_cg6565
adi_boardtype_cg6565c
adi_boardtype_unknown
adi_boardtype_xxx
adi_c_bit 1 2 3 4
adi_callctl_parms
adi_callprog_parmid
adi_callprog_parms 1 2 3
adi_cc_allmedia
adi_cc_autodtmf
adi_cc_autoecho
adi_cc_resvclrdwn
adi_cc_resvdtmf
adi_cc_resvsilence
adi_cc_state_connected 1 2
adi_cc_state_idle
adi_cleardown_parms
adi_collect_parmid 1 2 3
adi_collect_parms 1 2 3
adi_collect_quietly
adi_context_info 1 2
adi_cp_voice_
adi_cp_voice_begin 1 2
adi_cp_voice_end 1 2
adi_cp_voice_extended 1 2
adi_cp_voice_long 1 2
adi_cp_voice_medium 1 2
adi_cpmsk_precise_425
adi_cpmsk_precise_busy
adi_cpmsk_precise_ced
adi_cpmsk_precise_nu
adi_cpmsk_precise_sit
adi_cpmsk_precise_sitext 1 2
adi_cpmsk_precise_tdd
adi_cpstop_on_voice_begin
adi_d_bit 1 2 3 4
adi_dial_parms 1 2 3
adi_digit_0
adi_digit_1
adi_digit_2
adi_digit_3
adi_digit_4
adi_digit_5
adi_digit_6
adi_digit_7
adi_digit_8
adi_digit_9
adi_digit_a
adi_digit_all
adi_digit_any 1 2
adi_digit_b
adi_digit_c
adi_digit_d
adi_digit_pound
adi_digit_star
adi_ds0
adi_dtmf_parms 1 2 3
adi_dtmf_xxx
adi_dtmfdetect_parms 1 2 3 4
adi_echocancel_no_adapt
adi_echocancel_parms 1 2
adi_echocancel_parms echoparms
adi_echocancel_status_info 1 2 3
adi_eeprom_data
adi_encode
adi_encode_alaw 1 2 3 4 5
adi_encode_edtx 1 2
adi_encode_edtx_alaw
adi_encode_edtx_amrnb
adi_encode_edtx_evrc_fr_hdr_free 1 2
adi_encode_edtx_g723 1 2
adi_encode_edtx_g723_5 1 2
adi_encode_edtx_g723_6 1 2
adi_encode_edtx_g726
adi_encode_edtx_g729a
adi_encode_edtx_mu_law
adi_encode_edtx_mulaw
adi_encode_evrc_fr 1 2
adi_encode_g723_5 1 2 3
adi_encode_g723_6 1 2 3
adi_encode_g726 1 2
adi_encode_g726_16 1 2
adi_encode_g726_24 1 2
adi_encode_g726_32 1 2
adi_encode_g726_40 1 2
adi_encode_g729a 1 2
adi_encode_gsm 1 2
adi_encode_ima_24 1 2
adi_encode_ima_32 1 2
adi_encode_mulaw 1 2 3 4 5
adi_encode_nms_16 1 2 3
adi_encode_nms_24 1 2 3 4 5
adi_encode_nms_32 1 2 3
adi_encode_nms_64 1 2 3
adi_encode_oki_24 1 2
adi_encode_oki_32 1 2
adi_encode_pcm11m16 1 2
adi_encode_pcm11m8 1 2
adi_encode_pcm8m16 1 2 3 4 5
adi_encode_vox_32 1 2
adi_encoding_xxx
adi_energy_parms 1 2 3
adi_fskreceive_parms 1 2 3
adi_fsksend_parms 1 2 3
adi_full_duplex 1 2 3 4
adi_ivr_only
adi_lastbuffer_submitted
adi_max_digits
adi_mf_ccitt_backward
adi_mf_ccitt_forward
adi_mf_us
adi_native 1 2
adi_native_control 1 2
adi_native_parms
adi_play_last_buffer 1 2 3 4
adi_play_parms 1 2 3 4 5 6 7
adi_play_status
adi_play_underrun
adi_reason_
adi_reason_bad_stop_bit 1 2
adi_reason_drop_in_data 1 2
adi_record 1 2 3 4
adi_record_buffer_req 1 2 3 4
adi_record_parmid 1 2
adi_record_parms 1 2 3 4 5 6
adi_record_status
adi_record_underrun 1 2
adi_signal_duplex 1 2
adi_signal_input
adi_signal_output
adi_start 1 2
adi_start_parms 1 2 3 4 5
adi_state_started
adi_timeslot 1 2
adi_timeslot32
adi_tone_parms 1 2 3
adi_tonedetect_parms 1 2 3
adi_voice_duplex 1 2 3 4 5
adi_voice_input 1 2
adi_voice_output 1 2
adi_x_bit_
adiapi
adiassertsignal 1 2 3 4
adicallprogress
adicollectdigits 1 2 3 4 5 6 7 8 9 10 11
adicommandechocanceller 1 2
adicommandrecord 1 2 3 4 5 6 7
adidef 1 2 3 4 5 6 7 8 9 10 11
adidef.h 1 2 3 4
adierr_ 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16
adierr_cannot_create_channel 1 2
adierr_invalid_call_state 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20
adierr_invalid_queueid 1 2
adierr_no_dsp_port 1 2
adierr_no_dsp_resources 1 2
adierr_not_enough_resources 1 2
adierr_playrec_access 1 2 3 4
adierr_too_many_buffers 1 2 3 4 5
adierr_unknown_boardtype 1 2
adierr_xxx_xxx 1 2
adieven_play_done
adieven_record_done
adievn_
adievn_board_error 1 2 3 4
adievn_board_event 1 2 3
adievn_call_disconnected
adievn_collection_done 1 2 3 4 5 6
adievn_cp_busytone 1 2 3 4 5
adievn_cp_ced 1 2 3 4 5 6
adievn_cp_dialtone 1 2 3 4 5 6
adievn_cp_done 1 2 3 4 5 6 7
adievn_cp_noanswer 1 2 3 4 5
adievn_cp_reordertone 1 2 3 4 5
adievn_cp_ringquit 1 2 3 4 5
adievn_cp_ringtone 1 2 3 4 5
adievn_cp_rordtone
adievn_cp_sit 1 2 3 4 5
adievn_cp_stopped
adievn_cp_tdd 1 2
adievn_cp_voice 1 2 3 4 5
adievn_cp_voice_begin 1 2
adievn_cp_voice_end 1 2
adievn_cp_voice_extended 1 2
adievn_cp_voice_long 1 2
adievn_cp_voice_medium 1 2
adievn_dial_done 1 2 3 4 5
adievn_digit_begin 1 2 3 4 5 6 7 8
adievn_digit_end 1 2 3 4 5 6 7 8
adievn_dtmf_detect_done 1 2 3 4 5
adievn_dtmfdetect_done
adievn_echocancel_status 1 2 3 4 5
adievn_echocancel_tone 1 2 3 4
adievn_energy_detect_done 1 2 3 4 5 6
adievn_energy_detected 1 2 3 4 5
adievn_energydetect_done
adievn_fsk_receive_done 1 2 3 4 5 6
adievn_fsk_send_done 1 2 3 4 5
adievn_mf_detect_done 1 2 3 4 5
adievn_mf_digit_begin 1 2 3 4
adievn_mf_digit_end 1 2 3 4
adievn_play_buffer_req 1 2 3 4 5 6 7
adievn_play_done 1 2 3 4 5 6 7 8 9 10 11 12
adievn_pulse_done 1 2 3 4
adievn_query_energy_done
adievn_query_signal_done 1 2 3 4
adievn_record_buffer_full 1 2 3 4 5 6 7 8
adievn_record_done 1 2 3 4 5 6 7 8 9 10
adievn_record_event 1 2 3 4
adievn_record_started 1 2 3 4 5 6 7
adievn_recording_done
adievn_signal_detect_done 1 2 3 4 5
adievn_signalbit_changed 1 2 3 4
adievn_silence_detected 1 2 3 4 5
adievn_something_happened
adievn_startprotocol_done 1 2 3 4 5
adievn_stopprotocol_done 1 2 3 4
adievn_timer_done 1 2 3 4 5 6
adievn_timer_tick 1 2 3 4 5
adievn_tone_
adievn_tone_1_begin 1 2 3 4
adievn_tone_1_detect_done 1 2 3 4 5
adievn_tone_1_end 1 2 3 4
adievn_tone_2_begin 1 2 3 4
adievn_tone_2_detect_done 1 2 3 4 5
adievn_tone_2_end 1 2 3 4
adievn_tone_3_begin 1 2 3 4
adievn_tone_3_detect_done 1 2 3 4 5
adievn_tone_3_end 1 2 3 4
adievn_tone_4_begin 1 2 3 4
adievn_tone_4_detect_done 1 2 3 4 5
adievn_tone_4_end 1 2 3 4
adievn_tone_5_begin 1 2 3 4
adievn_tone_5_detect_done 1 2 3 4 5
adievn_tone_5_end 1 2 3 4
adievn_tone_6_begin 1 2 3 4
adievn_tone_6_detect_done 1 2 3 4 5
adievn_tone_6_end 1 2 3 4
adievn_tones_done 1 2 3 4 5 6
adievn_xxx_xxx 1 2
adievn_xxx in 'adidef
adiflushdigitqueue 1 2 3 4 5 6 7 8 9
adigetboardinfo 1 2 3 4 5 6
adigetboardslots 1 2 3 4
adigetboardslots32 1 2
adigetcontextinfo 1 2
adigetdigit 1 2 3 4 5 6 7 8 9
adigeteepromdata 1 2 3 4
adigetencodinginfo 1 2 3 4 5 6 7 8 9 10
adigetplaystatus 1 2 3 4 5 6 7
adigetrecordstatus 1 2 3 4 5 6
adigettimestamp 1 2 3 4 5 6
adiinsertdigit 1 2 3
adilps
adimgr 1 2
adimodifyechocanceller 1 2 3 4 5
adimodifyplaygain 1 2 3 4 5 6 7
adimodifyplayspeed 1 2 3 4 5 6 7
adipeekdigit 1 2 3 4 5 6
adiplay_access
adiplayasync 1 2 3 4 5 6 7 8 9 10 11 12 13 14
adiplayfrommemory 1 2 3 4 5 6 7 8 9 10 11 12 13 14
adiqueryenergy 1 2
adiquerysignalstate 1 2 3 4 5 6
adirecord_access
adirecordasync 1 2 3 4 5 6 7 8 9 10 11 12 13 14
adirecordtomemory 1 2 3 4 5 6 7 8 9 10 11
adisetboardclock 1 2
adisetnativeinfo 1 2 3 4 5 6 7 8 9 10
adistart_parms
adistartcallprogress 1 2 3 4 5 6 7
adistartdial 1 2 3 4 5 6 7 8 9
adistartdtmf 1 2 3 4 5 6 7 8 9 10
adistartdtmfdetector 1 2 3 4 5 6 7
adistartenergydetector 1 2 3 4 5 6 7 8 9 10
adistartmfdetector 1 2 3 4 5 6
adistartplaying 1 2 3 4 5 6 7 8 9 10 11 12 13 14
adistartprotocol 1 2 3 4 5 6 7 8 9 10 11
adistartpulse 1 2 3 4 5
adistartreceivingfsk 1 2 3 4 5 6
adistartrecording 1 2 3 4 5 6 7 8 9 10 11
adistartsendingfsk 1 2 3 4 5 6
adistartsignaldetector 1 2 3 4 5 6
adistarttimer 1 2 3 4 5
adistarttonedetector 1 2 3 4 5 6
adistarttones 1 2 3 4 5 6 7
adistopcallprogress 1 2 3
adistopcollection 1 2 3 4 5 6 7
adistopdial 1 2 3 4
adistopdtmfdetector 1 2 3 4 5 6
adistopenergy
adistopenergydetector 1 2 3 4
adistopmfdetector 1 2 3
adistopplaying 1 2 3 4 5 6 7 8 9 10 11
adistopprotocol 1 2
adistopreceivingfsk 1 2 3 4
adistoprecording 1 2 3 4 5 6 7 8 9 10
adistopsendingfsk 1 2 3 4
adistopsignaldetector 1 2 3 4
adistoptimer 1 2 3 4
adistoptonedetector 1 2 3 4
adistoptones 1 2 3 4 5
adisubmitplaybuffer 1 2 3 4 5
adisubmitrecordbuffer 1 2 3 4 5
adjusted 1 2
adjustment
administrative
adpcm 1 2
adsi 1 2
adsir 1 2
adsir_j 1 2
adsix 1 2
adsix_j
advance 1 2
advances
advantages 1 2
advisory 1 2

>>