<?xml version="1.0" encoding="UTF-8"?>
<ck><di ky="123" rd="receiving_billing_indications.htm|Receiving billing indications" ct=" Receiving billing indications  In any outbound call state, the application may receive NCCEVN ..."/><di ky="124" rd="receiving_overlapped_digits.htm|Receiving overlapped digits" ct=" Receiving overlapped digits  Some protocols support overlapped receiving of digits: the appli ..."/><di ky="125" rd="rejecting_calls.htm|Rejecting calls" ct=" Rejecting calls  To reject a call, an application invokes   nccRejectCall .  With most protoc ..."/><di ky="126" rd="repeat_dial_functions.htm|Repeat dial functions" ct=" Repeat dial functions        Function    Synchronous/ Asynchronous   ..."/><di ky="127" rd="revision_history.htm|Revision history" ct=" Revision history  	 	 	 	 		 Revision 		 Release date 		 Notes 	 	 		 900 ..."/><di ky="128" rd="running_nccxfer.html|Running nccxfer" ct=" Running nccxfer  nccxfer  demonstrates rerouting an incoming call.  Usage  nccxfer [ opti ..."/><di ky="129" rd="sending_billing_information.htm|Sending billing information" ct=" Sending billing information  In any incoming call state, the application can invoke  nccSetBi ..."/><di ky="130" rd="sending_overlapped_digits.htm|Sending overlapped digits" ct=" Sending overlapped digits  Some signaling protocols such as ISDN support overlapped sending o ..."/><di ky="131" rd="sending_protocolspecific_information.html|Sending protocol-specific information" ct=" Sending protocol-specific information  An application can  send protocol-specific information ..."/><di ky="132" rd="setting_call_control_mask_parameters.htm|Setting call control mask parameters" ct=" Setting call control mask parameters  The call control connectmask and disconnectmask paramet ..."/><di ky="133" rd="setting_up_the_naturalaccess_environment.htm|Setting up the NaturalAccess environment" ct="  Setting up the NaturalAccess environment  Before you can call functions from the NCC lib ..."/><di ky="134" rd="status_and_protocol_capability_functions_.htm|Status and protocol capability functions" ct=" Status and protocol capability functions        Function    Synchronous/  ..."/><di ky="135" rd="telephony_protocol_functions_.htm|Telephony protocol functions" ct=" Telephony protocol functions        Function    Synchronous/ Asynchronous ..."/><di ky="136" rd="terminology.htm|Terminology" ct=" Terminology  Note:  The product to  which this document pertains is part of the NMS Communi ..."/><di ky="137" rd="the_connected_call_state_.htm|The connected call state" ct="  The connected call state  In the connected call state, a connection exists between the c ..."/><di ky="138" rd="transferring_calls_.htm|Transferring calls" ct=" Transferring calls  The NCC API supports the ability to transfer calls from a first party to  ..."/><di ky="139" rd="using_the_event_reference.html|Using the event reference" ct=" Using the event reference  A typical event description includes:       Descriptio ..."/><di ky="140" rd="using_the_function_reference.htm|Using the function reference" ct=" Using the function reference  This section provides an alphabetical reference to the NCC API  ..."/><di ky="141" rd="using_webhelp.htm|Using WebHelp" ct=" Using WebHelp  To view this manual with full functionality, use one of the following browsers ..."/><di ky="142" rd="welcome.htm|Welcome" ct=" Dialogic® NaturalAccess™ NaturalCallControl™ API Developer’s Manual  This manual describes how  ..."/></ck>