# Fusion API and the CG 6060 board

Gateway applications provide a way of transferring data between telephone network and packet network interfaces. Fusion provides the ability to develop IP telephony gateway applications that run on CG boards. For more information about Fusion CG 6060 board configurations, refer to the Dialogic® NaturalAccess™ Fusion™ VoIP API Developer's Manual.

Fusion configurations use CG 6060 boards to receive and transmit data to PSTN and to IP networks. Fusion applications use NaturalCallControl API (NCC API) functions to place and receive PSTN calls, and Media Stream Protocol Processing API (MSPP API) functions to create and configure media channels between PSTN and IP networks. For more information about MSPP API functions, refer to the Dialogic® NaturalAccess™ Fusion™ Media Stream Protocol Processing API Developer's Manual.