# NetworkInterface.T1E1[x].Length

Specifies the length (in feet) of the cable connecting the board to the network so that the framer can adjust the pulse shape accordingly. Only applicable in T1 mode.

#### Syntax

NetworkInterface.T1E1[x].Length = length

x = 0-(n-1) (0-based trunk number or range of trunk numbers where n equals the number of trunks on the board.)

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0 - 655 (feet)

#### Example

NetworkInterface.T1E1[0..3].Length = 0

#### See also

NetworkInterface.T1E1[x].CRCMFMode, NetworkInterface.T1E1[x].D_Channel, NetworkInterface.T1E1[x].FrameType, NetworkInterface.T1E1[x].Impedance, NetworkInterface.T1E1[x].LineCode, NetworkInterface.T1E1[x].SignalingType, NetworkInterface.T1E1[x].Type