# Cabling the signal entry panel

The cables used to connect to the signal entry panel (SEP) vary based on the interface type on the board you are connecting.

The following illustrations show the cabling used to connect Dialogic® MD1 RJ-21 interfaces and Dialogic® MD1 Mini RJ-21 interfaces to the Dialogic SEP.

## Cabling boards with Dialogic® MD1 RJ-21 interfaces

## Cabling boards with Dialogic® MD1 Mini RJ-21 interfaces

## Signal entry panel kits

Dialogic offers the following kits containing signal entry panels and cables:

Description | Part number | Contents
SEP/cable kit – 1X (MD1 RJ-21 to (8) RJ-48C interface), 1U | 82923-1 | One SEP (P/N 83252) and one MD1 RJ-21 to MD1 RJ-21 cable (P/N 83225)
SEP/cable kit – 2X (MD1 RJ-21 to (8) RJ-48C interface), 1U | 82923-2 | One SEP (P/N 83252) and two MD1 RJ-21 to MD1 RJ-21 cables (2 x P/N 83225)
SEP/cable kit – 1X (MD1 MRJ-21 to (8) RJ-48C interface), 1U | 82924-1 | One SEP (P/N 83252) and one MD1 Mini RJ-21 to MD1 RJ-21 cable (P/N 83226)
SEP/cable kit – 2X (MD1 MRJ-21 to (8) RJ-48C interface), 1U | 82924-2 | One SEP (P/N 83252) and two MD1 Mini RJ-21 to MD1 RJ-21 cables (2 x P/N 83226)