# DSP.C5x[x].Image

Specifies a pre-linked DSP image file for CG 6565 boards.

#### Syntax

DSP.C5x[x].Image = filename

x = 0-(n-1) (A range of DSP cores where n equals the total number of DSP cores available.)

#### Access

Read/Write

#### Type

File name

#### Default

None.

#### Allowed values

Valid DSP image file name.

#### Example

DSP.C5x[1].Image = name.c41

#### Details

Use this keyword to specify DSP images that you create. The naming convention for DSP image files is filename.c41.

Setting DSP.C5x[x].Image = NULL leaves the specified DSPs in an unbooted state.

#### See also

DSP.C5x[x].Libs[y], DSP.C5x[x].OS, DSP.C5x[x].NumRxTimeSlots, DSP.C5x[x].NumTxTimeSlots, DSP.C5x[x].XLaw