<<

ns 1 2 3 4
ns_accept_unknown_fac_ie 1 2
ns_behaviour 1 2 3
ns_behaviour_nil 1 2
ns_call_proc_in
ns_disable_restart 1 2
ns_explicit_interface_id
ns_ie_relay_behaviour 1 2
ns_no_b_channel_management
ns_no_status_on_inv_op_ie
ns_no_status_on_unknown_ie
ns_pbx_xy
ns_pbx_xy_alternate
ns_preserve_ext_bit_in_chan_id
ns_relay
ns_send_user_connect_ack
ns_setup_ack_in
nsap 1 2
nsf 1 2 3 4
nt 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37
nt1
nt2
ntt 1 2 3 4
ntt_t300
ntt_t301
ntt_t303
ntt_t305
ntt_t306
ntt_t307
ntt_t308
ntt_t309
ntt_t310
ntt_t312
ntt_t313
ntt_t314
ntt_t316
ntt_t317
ntt_t318
ntt_t319
ntt_t322
ntt_t3ja
ntt_t_last 1 2
nuclear
null 1 2 3 4 5 6 7 8
number 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62
number of digits needed to route when
numerical
o 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34
oam 1 2 3 4 5 6 7 8 9 10
oamevn
oammon 1 2 3 4 5 6
oamsys 1 2 3
oamtrace
object 1 2 3 4 5 6 7
objhd
observation 1 2
observation period for frame error count 1 2
obtained 1 2 3 4 5
occurred 1 2 3 4 5 6 7 8 9 10
occurrence 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18
occurrences 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18
octet 1 2 3 4 5
octet_number
octet 3
octet 3.2
octet 3.3
octet 4
octet 4 etc
octet 5
october
odd 1 2 3 4 5

>>