# linemon syntax

linemon is installed in the C:\nms\bin\ directory in Windows or the /opt/nms/bin/ directory in UNIX.

linemon uses the following syntax:

linemon argument [argument]...

where:

Argument | Description
-b board | Specifies the board number to record. The default board number is 0.
-d | Display recorded data to the screen.
-e | Uses E1 mode, which assumes each trunk has 30 timeslots. If neither -e nor -E is specified, linemon uses T1 mode.
-E | Uses E1 raw mode, which assumes each trunk has 31 timeslots.
-f filename | Specifies a prefix for the record files. The default prefix is line.
-h | Prints a Help menu.
-l timeslot | Specifies a timeslot on the T1 or E1 trunk to be monitored. The default timeslot is 0.
-n timeslot | Specifies the DSP MUX timeslot to which the T1 or E1 trunk is connected. The default timeslot is 0.
-m timeslot | Specifies the DSP timeslot to use for monitoring. The default timeslot is 144.