# Video Messaging Server Interface overview

The Video Messaging Server Interface provides an application with a set of media processing capabilities for video and audio streams in an IPv4 or IPv6 network. These capabilities enable an application to play and record RTP audio and video streams, and to store data and retrieve data from 3GP file format files.

For information about the Video Messaging Server Interface components, architecture, and data flow, see the Video Access Overview Manual.