# Error types 9900

The following table lists the 9900 (digital line and clocking) errors:

Error code | Error name | Description | Category
--- | --- | --- | ---
-2049 | AGLCERR_LOCK_FAILED | Failed to wait for a resource. | 3
-2050 | AGLCERR_UNLOCK_FAILED | Failed to unload a semaphore. | 3
-2051 | AGLCERR_NOT_READY | Interrupt processing failed. | 3
-2055 | AGLCERR_INVALID_TRUNK | Trunk is out of range. | 3
-2056 | AGLCERR_INVALID_CHANNEL | Tried to configure a channel which is out of range. | 3
-2057 | AGLCERR_LOOPBACK_NOT_SUPPORTED | Requesting a loopback is an error since framer does not support per channel loopback. | 3
-2058 | AGLCERR_CANNOT_CHANGE_FRAME | Frame type cannot be changed on the fly. | 3
-2059 | AGLCERR_INVALID_PARAMETER | Invalid parameter passed to configuration functions (for example, framer, line code, line type). | 3
-2060 | AGLCERR_ASSERT | Received unexpected messages. | 3
-2061 | AGLCERR_MONITOR_DELAY | Interrupt processing procedure takes more than one second. | 3
-2062 | AGLCERR_MONITOR_FAILED | Lock failed more than two times. Monitor task should exit. | 3
-2063 | AGLCERR_REG_CHECK_FAILED | Reading indirect base returned an unexpected value. | 3
-2064 | AGLCERR_POLL_FAILED | Not used. | 3
-2065 | AGLCERR_UNEXPECTED_INTERRUPT | Received an unexpected E1/T1 interrupt while processing interrupts. | 3
-2066 | AGLCERR_UNKNOWN_BOARDTYPE | AGLC initialized with an unknown board type. | 3
-2067 | AGLCERR_IBCD_UNEXPECTED | Pertains to the second parameter. One of the following occurred: Already activated. Missed assert. Loopback not activated. Missed assert. Do not deactivate because may have received a deassert deactivate at the same time as an assert activate (if the two interrupts came at the same time). | 3
-2068 | AGLCERR_LOOPBACK_FAILED | Failed to configure loopback. | 3
-2069 | AGLCERR_LOOPBACK_CONFLICT | Loopback already exists. | 3
-2070 | AGLCERR_TOO_MANY_INTERRUPTS | More interrupts than can be handled. | 3
-2071 | AGLCERR_PARAM_FILE_CONFLICT | Parameter file conflict. Second parameter is ((option << 16) | T1/E1_RCV_OPT_VERSION_NUMBER)). | 3
-2072 | AGLCERR_INVALID_BER_THRESHOLDS | BER alarm threshold is less than BER alarm off threshold. | 3
-2073 | AGLCERR_MONITOR_RUNNING | AGLC manager error. Monitor already running. | 3
-2074 | AGLCERR_MONITOR_INACTIVE | AGLC manager error. Monitor currently inactive. | 3
-2075 | AGLCERR_SEND_FAILED | Received an unexpected E1/T1 interrupt while processing interrupts. | 3
-2077 | AGLCERR_BAD_PARM_COUNT | Alarm registration failed. Wrong parameter count. | 3
-3072 | HMICERR_LIBRARY_NOT_USABLE | Not used. | 3
-3073 | HMICERR_LIBRARY_NOT_INITIALIZED | Not used. | 3
-3074 | HMICERR_LOCK_CREATION_FAILED | Could not create AMX resource semaphore for HMIC. | 3
-3075 | HMICERR_LOCK_FAILED | Could not lock HMIC resource semaphore. | 3
-3076 | HMICERR_UNLOCK_FAILED | Failed to unlock HMIC resource semaphore. | 3
-3077 | HMICERR_DELAY_FAILED | Frame delay failed. | 3
-3078 | HMICERR_CONNECT_REFERENCE_CNT | Not used. | 3
-3079 | HMICERR_INVALID_BUS | Bus is invalid. | 3
-3080 | HMICERR_INVALID_STREAM | Stream is invalid. | 3
-3081 | HMICERR_INVALID_TIMESLOT | Timeslot is invalid. | 3
-3082 | HMICERR_INVALID_CLOCK_PARM | Not used. | 3
-3083 | HMICERR_INVALID_MODE | Framed connect mode is invalid if MVIP is in connect mode, and vice versa. | 3
-3084 | HMICERR_INVALID_PARAMETER | Physical address received as source while breaking connection. | 3
-3085 | HMICERR_NO_PATH | Failed to make a connection to DSP driver. | 3
-3086 | HMICERR_SWICH_VERIFY_FAILED | Switch number passed from the DSP driver is greater than number of secondary HMICs. | 3
-3087 | HMICERR_CONNECT_NOT_SUPPORTED | This error is returned if one of the following was true while making or breaking a mapping: Physical address is already mapped to a logical address. Mapping from one secondary HMIC to another. Mapping logical to logical. | 3
-3088 | HMICERR_MODE_NOT_SUPPORTED | HSEC8K_DRIVEN_BY_OSC mode for configuring sec8k clock is not supported. | 3
-3089 | HMICERR_MVIP_NOT_ENABLED | Failed to configure HMIC clock because MVIP is not enabled. | 3
-3090 | HMICERR_INVALID_MAP | Not used. | 3
-3091 | HMICERR_LOCAL_NOT_ENABLED | Local is not enabled. Informational message. | 3
-3092 | HMICERR_HW_INTERFACE_FAIL | Unknown mode (not framed connect or connect). | 3
-3093 | HMICERR_CONSUME_MESSAGE | Not used. | 3
-3110 | HMICERR_NO_RESOURCE | No free entries in HMIC mapping database. | 3
-3111 | HMICERR_INVALID_CLK_MAIN_SRC | Invalid clock source. | 3
-3112 | HMICERR_INVALID_CLK_FBK_SRC | Invalid fallback source. | 3
-3113 | HMICERR_INVALID_CLK_NTREF1_SRC | Invalid NETREF1 source. | 3
-3114 | HMICERR_INVALID_CLK_NTREF2_SRC | Invalid NETREF2 source. | 3
-3115 | HMICERR_INVALID_CLK_MAIN_PATH | Invalid main clock path selection. | 3
-3116 | HMICERR_INVALID_CLK_FBK_PATH | Invalid fallback clock path selection. | 3
-3117 | HMICERR_INVALID_HMIC_REFERENCE | Invalid HMIC number. | 3
-3118 | HMICERR_CLOCK_UPDATE_BUSY | Unable to lock HMIC data. | 3
-3119 | HMICERR_UNKNOWN_H100_MASTER | Invalid selection for master mode. | 3
-3120 | HMICERR_UNKNOWN_FBK_MODE | Invalid selection for fallback mode. | 3
-3121 | HMICERR_UNKNOWN_LSCX_OUTPUT | Invalid LSCX stream. | 3
-3122 | HMICERR_UNKNOWN_LSCX_CHOICE | Invalid LSCX signal. | 3
-3123 | HMICERR_UNKNOWN_FG_PIN_CFG | Invalid frame group configuration. | 3
-3124 | HMICERR_UNKNOWN_FG_SPEED | Invalid frame group speed. | 3
-3125 | HMICERR_UNKNOWN_FG_WIDTH | Invalid frame group width. | 3
-3126 | HMICERR_UNRECOGNIZED_REG | Invalid register. | 3