# NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Board

Specifies the board number (as defined in oamsys.cfg) on which this NFAS member resides.

#### Syntax

NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Board = setting

x = 0-(n-1) (0-based trunk number or range of trunk numbers where n equals the number of trunks on the board.)

y = index of the NFAS group member

#### Access

Read/Write

#### Type

Integer

#### Default

For every member of an NFAS group, this keyword must be set in the board keyword file of the board where the D channel resides.

#### Allowed values

Any board number, as defined in the OAM system configuration file oamsys.cfg.

#### Example

NetworkInterface.T1E1[0].ISDN.NFAS_Member[1].Board = 0

#### Details

This board number must match the board number specified in the OAM system configuration file.

When using this keyword, NetworkInterface.T1E1[x].D_Channel must be set to ISDN for the trunk (x) bearing the primary D channel.

For information about the system configuration file, refer to the Dialogic® NaturalAccess™ OAM System Developer’s Manual. For information about configuring NaturalAccess ISDN Software, refer to the Dialogic® NaturalAccess™ ISDN Software Installation Manual .

#### See also

NetworkInterface.T1E1[x].ISDN.D_Channel_Backup_Trunk, NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].NAI, NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Trunk, NetworkInterface.T1E1[x].ISDN.NFASGroup