<?xml version="1.0" encoding="UTF-8"?>
<ck><di ky="177" rd="resourcexdefinitions.html|Resource[x].Definitions" ct=" Resource[x].Definitions  Provides a relational string of data processing functions (DPFs) tha ..."/><di ky="178" rd="resourcexdsps.html|Resource[x].DSPs" ct="  Resource[x].DSPs  Specifies the DSPs associated with a resource  pool  (identified by  ..."/><di ky="179" rd="resourcexname.html|Resource[x].Name" ct="  Resource[x].Name  Specifies a name to associate with a resource  pool  (identified by  ..."/><di ky="180" rd="resourcexsize.html|Resource[x].Size" ct="  Resource[x].Size  Specifies the number of channels or ports for the  pool  reserved by ..."/><di ky="181" rd="resourcexstarttimeslot.html|Resource[x].StartTimeSlot" ct="  Resource[x].StartTimeSlot  Specifies the starting timeslot for a  pool .  Syntax  ..."/><di ky="182" rd="resourcextcps.html|Resource[x].TCPs" ct=" Resource[x].TCPs  Specifies the names of the TCPs used on the board to set up and tear down c ..."/><di ky="183" rd="retrieving_keyword_values.htm|Retrieving keyword values" ct=" Retrieving keyword values  To retrieve the values of read/write and read-only keywords:   ..."/><di ky="184" rd="revision_history.htm|Revision history" ct=" Revision history  	 	 	 	 		 Revision 		 Release date 		 Notes 	 	 		 900 ..."/><di ky="185" rd="running_in_ipv4_ipv6_dual_stack_mode.htm|Running in IPv4/IPv6 dual stack mode" ct="  Running in IPv4/IPv6 dual stack mode  CG boards implement an IPv4/IPv6 dual stack that a ..."/><di ky="186" rd="running_oamsys.htm|Running oamsys" ct=" Running oamsys  To run  oamsys , enter the following command from the command line:  oamsys ..."/><di ky="187" rd="sample_board_keyword_file.html|Sample board keyword file" ct=" Sample board keyword file  The following sample board keyword file for no call control (NOCC) ..."/><di ky="188" rd="setting_keyword_values.htm|Setting keyword values" ct=" Setting keyword values  There are several ways to set the values of read/write keywords:   ..."/><di ky="189" rd="setting_or_retrieving_the_acoustic_echo_control_state.htm|Setting or retrieving the acoustic echo control state" ct=" Setting or retrieving the acoustic echo control state  The acoustic echo control (AEC) stat ..."/><di ky="190" rd="setting_or_retrieving_the_echo_cancellation_bypass_state.htm|Setting or retrieving the echo cancellation bypass state" ct=" Setting or retrieving the echo cancellation bypass state  The bypass control allows you to  ..."/><di ky="191" rd="setting_or_retrieving_the_nonlinear_processing_state.htm|Setting or retrieving the nonlinear processing state" ct=" Setting or retrieving the nonlinear processing state  Nonlinear processing (NLP) removes re ..."/><di ky="192" rd="setting_up_multihomed_configurations.html|Setting up multi-homed configurations" ct=" Setting up multi-homed configurations  On CG boards, each Ethernet interface can be configure ..."/><di ky="193" rd="signaling.html|Signaling" ct=" Signaling  Two types of information are carried on a trunk:    Voice information   ..."/><di ky="194" rd="software_components.html|Software components" ct=" Software components  NaturalAccess  is a development environment  that provides such servic ..."/><di ky="195" rd="software_echo_cancellation_mips.htm|Software echo cancellation MIPS" ct=" Software echo cancellation MIPS  Use the CG 6565 daughterboard with an echo chip to provide e ..."/><di ky="196" rd="software_echo_cancellation_restriction.html|Software echo cancellation restriction" ct=" Software echo cancellation restriction  Only one software echo canceler runs per call. Theref ..."/><di ky="197" rd="specifying_configuration_file_locations.htm|Specifying configuration file locations" ct=" Specifying configuration file locations  Some board keywords require file names as parameters ..."/><di ky="198" rd="status_indicator_leds.html|Status indicator LEDs" ct=" Status indicator LEDs  The CG 6565 board contains three types of LEDs:    Trunk LEDs  ..."/><di ky="199" rd="switch_blocking.html|Switch blocking" ct=" Switch blocking  The CG 6565 board:    Can simultaneously connect (simplex) to all 4096 ..."/><di ky="200" rd="switchconnections.html|SwitchConnections" ct="  SwitchConnections  Specifies whether the board nails up default switch connections when  ..."/><di ky="201" rd="switchconnectmode.html|SwitchConnectMode" ct="  SwitchConnectMode  Specifies how switch connections are made on the board.  Syntax  ..."/><di ky="202" rd="system_requirements.html|System requirements" ct=" System requirements  To install and use CG 6565 boards, your system must have:    A cha ..."/><di ky="203" rd="temperature_and_fan_monitoring_system.htm|Temperature and fan monitoring system" ct=" Temperature and fan monitoring system  CG 6565 boards include a temperature and a fan monitor ..."/><di ky="204" rd="terminology.htm|Terminology" ct=" Terminology  Note:  The product to  which this document pertains is part of the NMS Communi ..."/><di ky="205" rd="testing_in_loopback_mode.htm|Testing in loopback mode" ct=" Testing in loopback mode  Connect the CG 6565 board in loopback mode to test the digital trun ..."/><di ky="206" rd="tpktcomplexforward.count.html|TPKT.ComplexForward.Count" ct="  TPKT.ComplexForward.Count  Specifies the number of condition sets for the system when send ..."/><di ky="207" rd="tpktcomplexforwardxdestinationpacketsize.html|TPKT.ComplexForward[x].DestinationPacketSize" ct="  TPKT.ComplexForward[x].DestinationPacketSize  Specifies the amount of  packet  data (in by ..."/><di ky="208" rd="tpktcomplexforwardxlifetimeticks.html|TPKT.ComplexForward[x].LifeTimeTicks" ct="  TPKT.ComplexForward[x].LifeTimeTicks  Specifies the number of 10 millisecond timer ticks t ..."/><di ky="209" rd="tpktcomplexrxport.html|TPKT.ComplexRxPort" ct="  TPKT.ComplexRxPort  Specifies a UDP port number on which to receive complex ThroughPacke ..."/><di ky="210" rd="tpktcomplextxport.html|TPKT.ComplexTxPort" ct="  TPKT.ComplexTxPort  Specifies a UDP port number on which to transmit complex ThroughPack ..."/><di ky="211" rd="tpktenable.html|TPKT.Enable" ct="  TPKT.Enable  Enables or disables ThroughPacket  packet  multiplexing functionality on  ..."/><di ky="212" rd="tpktnumberofcomplexforwardconditions.html|TPKT.NumberOfComplexForwardConditions" ct=" TPKT.NumberOfComplexForwardConditions  Specifies the number of conditions specified for Throu ..."/><di ky="213" rd="tpktsimplerxport.html|TPKT.SimpleRxPort" ct="  TPKT.SimpleRxPort  Specifies a valid UDP port number on which to receive simple ThroughP ..."/><di ky="214" rd="tpktsimpletxport.html|TPKT.SimpleTxPort" ct="  TPKT.SimpleTxPort  Specifies a UDP port number on which to transmit simple ThroughPacket ..."/><di ky="215" rd="trunk_control_program_resource_usage.html|Trunk control program resource usage" ct=" Trunk control program resource usage  The  Resource[x].TCPs  keyword specifies which TCPs are ..."/><di ky="216" rd="trunk_interfaces.htm|Trunk interfaces" ct=" Trunk interfaces  A CG 6565 board has either  four-trunks   or  eight-trunks .  	 	  ..."/><di ky="217" rd="using_board_keyword_files.htm|Using board keyword files" ct=" Using board keyword files  A board keyword file contains a list of parameters to configure a  ..."/><di ky="218" rd="using_echo_cancellation_control.html|Using echo cancellation control" ct=" Using echo cancellation control  The CG 6565 board includes a hardware echo cancellation feat ..."/><di ky="219" rd="using_the_keyword_reference.html|Using the keyword reference" ct=" Using the keyword reference  The keywords are presented in detail in the following topics. Ea ..."/><di ky="220" rd="using_webhelp.htm|Using WebHelp" ct=" Using WebHelp  To view this manual with full functionality, use one of the following browsers ..."/><di ky="221" rd="utility_summary.htm|Utility summary" ct=" Utility summary  This section provides detailed information about the following CG 6565 board ..."/><di ky="222" rd="verifying_the_board_installation.html|Verifying the board installation" ct=" Verifying the board installation  Complete the following steps to verify that you have instal ..."/><di ky="223" rd="verifying_trunk_connections.html|Verifying trunk connections" ct=" Verifying trunk connections  Complete the following steps to verify that the board is working ..."/><di ky="224" rd="versionmajor.html|Version.Major" ct=" Version.Major  Indicates the major version number of the CG plug-in.  Syntax  Version.Maj ..."/><di ky="225" rd="versionminor.html|Version.Minor" ct=" Version.Minor  Indicates the minor version number of the CG plug-in.  Syntax  Version.Min ..."/><di ky="226" rd="voice_encoding.html|Voice encoding" ct="  Voice encoding  For the CG 6565 board, the information received is already pulse code mo ..."/><di ky="227" rd="welcome.htm|Welcome" ct="  Dialogic® CG 6565 PCI Media Board Installation and Developer&apos;s Manual  The  Dialogic® CG 6 ..."/><di ky="228" rd="worstcase_resource_management_calculation.html|Worst-case resource management calculation" ct="  Worst-case resource management calculation  One way to find out if the available board r ..."/></ck>