<?xml version="1.0" encoding="UTF-8"?>
<ck><di ky="118" rd="glossary__stream.htm|Glossary: stream" ct=" A group of timeslots that usually corresponds to a particular bit-stream of time-domain multipl ..."/><di ky="119" rd="glossary__timeslot.htm|Glossary: timeslot" ct=" Information in each channel is time division multiplexed into a single continuous stream of dat ..."/><di ky="120" rd="glossary__zero_code_suppression.htm|Glossary: zero code suppression" ct=" The insertion of a one bit to prevent the transmission of eight or more consecutive zero bits.  ..."/><di ky="121" rd="glossary_tsi.htm|Glossary: TSI" ct=" Transmitting subscriber identification; used by the transmitting fax terminal to identify itsel ..."/><di ky="122" rd="hardwareecho.echochipenabled.htm|HardwareEcho.EchoChipEnabled" ct=" HardwareEcho.EchoChipEnabled  Enables or disables the echo cancellation hardware.  Syntax ..."/><di ky="123" rd="hardwareecho.trunk_x_.onofftimeslots.htm|HardwareEcho.Trunk[x].OnOffTimeslots" ct=" HardwareEcho.Trunk[x].OnOffTimeslots  Enables or disables hardware echo cancellation by tru ..."/><di ky="124" rd="hardwareecho.xlaw.htm|HardwareEcho.XLaw" ct=" HardwareEcho.XLaw  Determines the echo hardware companding mode.  Syntax  HardwareEcho. ..."/><di ky="125" rd="hdlcxboot.html|Hdlc[x].Boot" ct="  Hdlc[x].Boot  Enables or disables the  HDLC  channel associated with a particular trun ..."/><di ky="126" rd="hdlcxrxtimeslot.html|Hdlc[x].RxTimeSlot" ct="  Hdlc[x].RxTimeSlot  Specifies the TDM timeslot of the receiving  HDLC  channel for a s ..."/><di ky="127" rd="hdlcxtxtimeslot.html|Hdlc[x].TxTimeSlot" ct="  Hdlc[x].TxTimeSlot  Specifies the TDM timeslot of the transmitting  HDLC  channel for  ..."/><di ky="128" rd="informational_keywords.html|Informational keywords" ct=" Informational keywords  This topic describes read-only keywords for retrieving information. D ..."/><di ky="129" rd="installation_summary.html|Installation summary" ct=" Installation summary  The following table summarizes the procedure for installing the hardwar ..."/><di ky="130" rd="installing_the_board.htm|Installing the board" ct=" Installing the board       Warning:     The CG 6565 board powers up and fun ..."/><di ky="131" rd="ipc.addroute_x_.vlantag.htm|IPC.AddRoute[x].VlanTag" ct=" IPC.AddRoute[x].VlanTag  Specifies a VLAN tag to be added to all packets sent to the IPv4 s ..."/><di ky="132" rd="ipcaddroutexdestinationaddress.html|IPC.AddRoute[x].DestinationAddress" ct="  IPC.AddRoute[x].DestinationAddress  Specifies the  IPv4  address of the Ethernet inter ..."/><di ky="133" rd="ipcaddroutexgatewayaddress.html|IPC.AddRoute[x].GatewayAddress" ct="  IPC.AddRoute[x].GatewayAddress  Specifies the  IPv4  address of the router.  Syntax ..."/><di ky="134" rd="ipcaddroutexinterface.html|IPC.AddRoute[x].Interface" ct="  IPC.AddRoute[x].Interface  Specifies the Ethernet interface (1 or 2) associated with  ..."/><di ky="135" rd="ipcaddroutexmask.html|IPC.AddRoute[x].Mask" ct="  IPC.AddRoute[x].Mask  Specifies a subnet mask for the  IPv4  address specified in  IPC ..."/><di ky="136" rd="ipv6.link_x_.enable.htm|IPv6.Link[x].Enable" ct="  IPv6.Link[x].Enable  Enables or disables  IPv6  on the specified Ethernet interface. F ..."/><di ky="137" rd="ipv6.link_x_.enableping.htm|IPv6.Link[x].EnablePing" ct="  IPv6.Link[x].EnablePing  Enables or disables  IPv6  PING on the specified Ethernet int ..."/><di ky="138" rd="ipv6.link_x_.hoplimit.htm|IPv6.Link[x].HopLimit" ct="  IPv6.Link[x].HopLimit  Specifies the default  IPv6   hop limit  value for the specif ..."/><di ky="139" rd="ipv6.link_x_.icmpratelimit.htm|IPv6.Link[x].ICMPRateLimit" ct="  IPv6.Link[x].ICMPRateLimit  Specifies the  IPv6   ICMP  rate limit for the specified ..."/><di ky="140" rd="ipv6.link_x_.ipsec.htm|IPv6.Link[x].IPSec" ct="  IPv6.Link[x].IPSec  Enables or disables  IPSec  for  IPv6  on the specified Ethernet ..."/><di ky="141" rd="ipv6.link_x_.mtu.htm|IPv6.Link[x].MTU" ct="  IPv6.Link[x].MTU  Sets the  IPv6  maximum transmission unit ( MTU ) for the specifie ..."/><di ky="142" rd="ipv6.link_x_.ndattempts.htm|IPv6.Link[x].NDAttempts" ct="  IPv6.Link[x].NDAttempts  Specifies the neighbor discovery attempt (NDA) limit for the sp ..."/><di ky="143" rd="ipv6.link_x_.ndreachabilitytimer.htm|IPv6.Link[x].NDReachabilityTimer" ct="  IPv6.Link[x].NDReachabilityTimer  Specifies the neighbor discovery reachability timer (i ..."/><di ky="144" rd="ipv6.link_x_.ndretrantimer.htm|IPv6.Link[x].NDRetranTimer" ct="  IPv6.Link[x].NDRetranTimer  Specifies the neighbor discovery retransmission timer (in mi ..."/><di ky="145" rd="keyword_types.html|Keyword types" ct=" Keyword types  The keywords for a CG 6565 board describe that board&apos;s configuration. Some key ..."/><di ky="146" rd="locationpcibus.html|Location.PCI.Bus" ct=" Location.PCI.Bus  Specifies the PCI logical bus location of the board.  Syntax  Location. ..."/><di ky="147" rd="locationpcislot.html|Location.PCI.Slot" ct=" Location.PCI.Slot  Defines the logical slot location of the board on the PCI bus.  Syntax  ..."/><di ky="148" rd="managed_dsp_resources.html|Managed DSP resources" ct=" Managed DSP resources  CG boards are based on a flexible software and hardware architecture.  ..."/><di ky="149" rd="managing_board_dsp_resources.html|Managing board DSP resources" ct="  Managing board DSP resources  This topic describes:  	 Setting 	 up a single resourc ..."/><di ky="150" rd="maxchannels.html|MaxChannels" ct="  MaxChannels  Specifies the maximum number of channels to allocate on the board. A channe ..."/><di ky="151" rd="migration_information.htm|Migration information" ct=" Migration information    The CG 6565 board is based on the CG 6000/C, CG 6100C, and CG 6500 ..."/><di ky="152" rd="monitoring_ethernet_link_status_events.html|Monitoring Ethernet link status events" ct=" Monitoring Ethernet link status events  The  oammon  utility displays Ethernet link status ev ..."/><di ky="153" rd="name.html|Name" ct=" Name  Specifies the name assigned to the CG 6565 board.  Syntax  Name =  board_name  Ac ..."/><di ky="154" rd="natural_access_media_masks_and_call_progress_masks.html|Natural Access media masks and call progress masks" ct="  Natural Access media masks and call progress masks  Natural Access uses a media mask and ..."/><di ky="155" rd="networkinterface.t1e1_x_.alarmmode.htm|NetworkInterface.T1E1[x].AlarmMode" ct=" NetworkInterface.T1E1[x].AlarmMode  For T1 interfaces, specifies if alarm conditions are de ..."/><di ky="156" rd="networkinterfaceethernetxmacaddress.html|NetworkInterface.Ethernet[x].MAC_Address" ct="  NetworkInterface.Ethernet[x].MAC_Address  Specifies the  MAC address .  Syntax  Ne ..."/><di ky="157" rd="networkinterfacet1e1xcrcmfmode.html|NetworkInterface.T1E1[x].CRCMFMode" ct=" NetworkInterface.T1E1[x].CRCMFMode  Specifies whether or not the board performs CRC signal ch ..."/><di ky="158" rd="networkinterfacet1e1xdchannel.html|NetworkInterface.T1E1[x].D_Channel" ct="  NetworkInterface.T1E1[x].D_Channel  Specifies whether the trunk has a primary  D chann ..."/><di ky="159" rd="networkinterfacet1e1xframetype.html|NetworkInterface.T1E1[x].FrameType" ct=" NetworkInterface.T1E1[x].FrameType  Defines the T1 or E1 trunk framing format for current boa ..."/><di ky="160" rd="networkinterfacet1e1ximpedance.html|NetworkInterface.T1E1[x].Impedance" ct=" NetworkInterface.T1E1[x].Impedance  Specifies the type of cable connecting a CG 6565 board to ..."/><di ky="161" rd="networkinterfacet1e1xisdndchannelbackuptrunk.html|NetworkInterface.T1E1[x].ISDN.D_Channel_Backup_Trunk" ct="  NetworkInterface.T1E1[x].ISDN.D_Channel_Backup_Trunk  Specifies the 0-based trunk to car ..."/><di ky="162" rd="networkinterfacet1e1xisdnnfasgroup.html|NetworkInterface.T1E1[x].ISDN.NFASGroup" ct="  NetworkInterface.T1E1[x].ISDN.NFASGroup  Specifies the  NFAS  group number.  Syntax ..."/><di ky="163" rd="networkinterfacet1e1xisdnnfasmemberyboard.html|NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Board" ct="  NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Board  Specifies the board number (as defin ..."/><di ky="164" rd="networkinterfacet1e1xisdnnfasmemberynai.html|NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].NAI" ct="  NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].NAI  Identifies the Network Access Identifi ..."/><di ky="165" rd="networkinterfacet1e1xisdnnfasmemberytrunk.html|NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Trunk" ct="  NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Trunk  Specifies the zero-based trunk numbe ..."/><di ky="166" rd="networkinterfacet1e1xlength.html|NetworkInterface.T1E1[x].Length" ct=" NetworkInterface.T1E1[x].Length  Specifies the length (in feet) of the cable connecting the b ..."/><di ky="167" rd="networkinterfacet1e1xlinecode.html|NetworkInterface.T1E1[x].LineCode" ct="  NetworkInterface.T1E1[x].LineCode  Specifies the  ones density  maintenance method used on ..."/><di ky="168" rd="networkinterfacet1e1xsignalingtype.html|NetworkInterface.T1E1[x].SignalingType" ct=" NetworkInterface.T1E1[x].SignalingType  Determines how voice and signaling information is rou ..."/><di ky="169" rd="networkinterfacet1e1xtype.html|NetworkInterface.T1E1[x].Type" ct=" NetworkInterface.T1E1[x].Type  Specifies the trunk type for each trunk on the board. This set ..."/><di ky="170" rd="notices.htm|Notices" ct=" Copyright and legal notices  Copyright © 2005-2010 Dialogic Corporation.  All Rights Reserv ..."/><di ky="171" rd="number.html|Number" ct=" Number  Specifies a logical board number for this board.  Syntax  Number =  board_number ..."/><di ky="172" rd="plugin_keywords.html|Plug-in keywords" ct=" Plug-in keywords  CG plug-in keywords provide specific board family information for CG boards ..."/><di ky="173" rd="pri_mode_switching.htm|PRI mode switching" ct="  PRI mode switching  This topic contains the following PRI mode switching information:   ..."/><di ky="174" rd="productsx.html|Products[x]" ct=" Products[x]  At the plug-in level, indicates the product supported by the plug-in.  Syntax ..."/><di ky="175" rd="raw_mode_switching.htm|RAW mode switching" ct="  RAW mode switching  This topic contains the following RAW mode switching information:   ..."/><di ky="176" rd="resource_definitions.html|Resource definitions" ct=" Resource definitions  This topic provides examples of  Resource[x].Definitions   strings th ..."/></ck>