# Current table

The following table summarizes the objects in the Trunk MIB Current table, otherwise known the dsx1CurrentEntry block of variables:

Object | Syntax | Description
--- | --- | ---
dsx1CurrentIndex | Integer | Number of the DS1 interface.
dsx1CurrentESs | Gauge | Number of errored seconds.
dsx1CurrentSESs | Gauge | Number of severely errored seconds.
dsx1CurrentSEFSs | Gauge | Number of severely errored framing seconds.
dsx1CurrentUASs | Gauge | Number of unavailable seconds.
dsx1CurrentCSSs | Gauge | Number of controlled slip seconds.
dsx1CurrentPCVs | Gauge | Number of path coding violations.
dsx1CurrentLESs | Gauge | Number of interface errored seconds.
dsx1CurrentBESs | Gauge | Number of bursty errored seconds.
dsx1CurrentDMs | Gauge | Number of degraded minutes.
dsx1CurrentLCVs | Gauge | Number of line code violations.