<<

adapt 1 2 3 4
adaptation 1 2
adapted
adapter 1 2 3
adapters
adaptive 1 2
add 1 2 3 4 5 6 7
added 1 2 3 4 5
adding 1 2 3 4
addition 1 2 3 4 5 6 7
additional 1 2 3 4 5 6 7 8 9 10
addr 1 2
address 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29
addresses 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17
addressing 1 2 3 4 5
addroute 1 2 3 4 5 6 7 8 9 10
adds 1 2 3 4 5
adi 1 2 3 4
adi_echocancel_parms
adi_encode_alaw 1 2
adi_encode_amr_102
adi_encode_amr_122
adi_encode_amr_475
adi_encode_amr_515
adi_encode_amr_59
adi_encode_amr_67
adi_encode_amr_74
adi_encode_amr_795
adi_encode_edtx_g729a
adi_encode_g723_5
adi_encode_g723_6
adi_encode_g723_edtx_g_723_5
adi_encode_g723_edtx_g_723_6
adi_encode_g726 1 2
adi_encode_g729a
adi_encode_gsm
adi_encode_ima_24
adi_encode_ima_32
adi_encode_mulaw 1 2
adi_encode_nms_16 1 2
adi_encode_nms_24 1 2
adi_encode_nms_32 1 2
adi_encode_nms_64 1 2
adi_encode_oki_24
adi_encode_oki_32
adi_encode_pcm11m16
adi_encode_pcm11m8
adi_encode_pcm8m16 1 2
adi_placecall
adi_start
adicommandrecord
adievn_record_buffer_full
adimodifyechocanceller
adirecordasync
adistartcallprogress
adistartdial
adistartdtmf
adistartdtmfdetector
adistartenergydetector
adistartmfdetector
adistartplaying
adistartprotocol
adistartreceivingfsk
adistartrecording
adistartsendingfsk
adistarttonedetector
adistarttones
adisubmitrecordbuffer
adjacent
adjust 1 2
administration
adp
adpcm 1 2 3 4
adsi
adsir 1 2 3
adsir_j
adsix 1 2 3
adsix_j
advert
advertisement
advertisements 1 2
aec
affect 1 2
affects
ag
again 1 2 3 4
agload 1 2 3
agreement
agsw
ah 1 2
airflow
ais 1 2
alarm 1 2 3 4 5 6 7
alarmmode
alarms 1 2
algorithm 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16
algorithms 1 2 3 4 5 6 7
alignment
allconstantdelay
alldirect
alliance 1 2 3
allocate 1 2 3 4 5 6
allocated 1 2 3 4 5 6 7 8 9
allocates 1 2 3
allocation 1 2 3 4 5 6 7 8
allow 1 2 3 4 5 6 7 8
allowable
allowed 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107
allowing 1 2 3
allows 1 2 3 4 5 6 7 8 9 10 11 12 13
along 1 2
alphabetically
already
alternate 1 2 3 4
alternately
alternative 1 2 3 4
although 1 2 3
altitude
always 1 2 3 4 5 6 7

>>