# TPKT.Enable

Enables or disables ThroughPacket packet
multiplexing functionality on the board.

#### Syntax

TPKT.Enable = value

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0 | 1

#### Example

TPKT.Enable = 1

#### Details

Set TPKT.Enable to 1 to enable ThroughPacket multiplexing. Set TPKT.Enable to 0 to disable ThroughPacket multiplexing.

For information about the Clarent ThroughPacket multiplexing algorithm and its implementation in Fusion software, refer to the Dialogic® NaturalAccess™ Fusion™ VoIP API Developer’s Manual.

#### See also

TPKT.ComplexRxPort, TPKT.ComplexTxPort