# FGD editable parameters

To program the FGD TCP to implement the specifications of the supported countries and network operators, modify the TCP-specific parameters stored within the parameter category NCC.X.ADI_FGD. You can modify parameters that program TCP/host interaction, configure unregulated features or configure features that can change from switch to switch within the same network.

The following table describes NCC.X.ADI_FGD parameters (within the parameter category NCC.X.ADI_FGD) that you can modify:

Field | Unit | Default | Description
--- | --- | --- | ---
optionflags | mask | 0x0 | Not used
sendanididwink | mask | 0x0 | If set, generate wink between ANI and DID digits.
expectanididwink | mask | 0x0 | If set, expect wink between ANI and DID digits.
expectfinalwink | mask | 0x1 | Determines if there is a final wink after digit reception: 0 - There will be a final wink. 1 - There will not be a wink.

Refer to FGD non-editable parameters for more information.