# snmpChassScan

Demonstrates how to:

- Navigate the chassis MIB.

- Retrieve chassis type and description.

- Navigate by bus.

- Show board description and status information.

#### Usage

snmpChassScan address options

where:

Parameter | Description
--- | ---
address | Address or DNS name of a local or remote host running the SNMP agent about which to return information.

Valid options include:

Option | Description
--- | ---
-ccommunity_name | Specify a community name. The default is public.
-rn | Number of retries. The default is 1 retry.
-tn | Timeout in hundredths of a second. The default is 100 (1 second).

Polling is set interactively by the application.

#### Procedure

Complete the following steps to run snmpChassScan:

Step | Action
1 | From the command line, navigate to the \nms\ctaccess\demos\snmp\snmpchassscan directory (or the /opt/nms/ctaccess/demos/snmp/snmpchassscan directory under UNIX)
2 | Enter the following command: snmpChassScan

The following example shows how to run snmpChassScan:

< snmpChassScan.exe
> SNMP Demonstration and Test Program V.3.0 Nov 15 1999
> NMS Communications Corporation.
>Usage:
>snmpChassScan [Address | DNSName] [options]
>Address: default is 127.0.0.1
>options: -cCommunity_name, specify community default is 'public'
> -rN , retries default is N = 1 retry
> -tN , timeout in hundredths-seconds default is N = 100 = 1 second
>
>H Help S Sys info L Board list P<N> Poll Interval Q Quit
>
>SEND A REQUEST FOR SYSTEM INFO TO: 10.1.20.45
>System information:
>System: Hardware: x86 Family 6 Model 3 Stepping 4 AT/AT COMPATIBLE - >Software: Windows 2000
>SysUpTime: 1:22:15.66
>SysContact: Joe Kilroy
>Computer name: KILROY
>Location: NMS
>
>SEND A REQUEST FOR NMS BOARDS TO: 10.1.20.45
> PCI bus
>Board 1: AG_4040_1TE Segment:1 Slot:7 Status:OnLine
>Board 2: AG_4040_2TE Segment:1 Slot:6 Status:OnLine
>