# TempSensor[x].CritThres

Specifies the critical threshold of a temperature sensor in tenth of a degree Celsius. There are four temperature sensors on the CG 6565C board.

#### Syntax

TempSensor[x].CritThres = temperature

x = 0 (index of the main temperature sensor)

x = 1 (index of the PPC temperature sensor)

x = 2 (index of the DSP temperature sensor)

x = 3 (index of the rear I/O transition board temperature sensor)

#### Access

Read/Write

#### Type

Integer

#### Default

Main temperature sensor = 750

PPC temperature sensor = 970

DSP temperature sensor = 750

Rear I/O transition board temperature sensor = 750

#### Allowed values

100 - 1200

#### Example

TempSensor[0].CritThres = 750

#### Details

The warning threshold temperature needs to be below the shutdown temperature, otherwise an OAM event is not received. The CG 6565C board has the following shutdown temperatures:

Main board sensor = 85° C

PPC sensor = 100° C

DSP sensor = 85° C

Rear board sensor = 85° C

#### See also

TempSensor[x].WarnThres