# ACU_NOTIFY_IN

This topic describes:

- ACU_NOTIFY_IN protocol variants

- ACU_NOTIFY_IN macro descriptions and Q.931 IE

#### Purpose

Indicates that a NOTIFY message was received.

#### Conn_id

An allocated call.

## ACU_NOTIFY_IN protocol variants

The following table lists the variants under which each macro is supported for this primitive. In this table, x indicates both NT and TE sides.

Macro | 4 E S S | E 1 0 | N I 2 | D M S | E T S I | V N 6 | H K G | A U S T E L 1 | N T T | K O R E A | T A I W A N | Q S I G | D P N S S | T 1 6 0 7
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acu_notify_in_a_connected_name, Acu_notify_in_connected_name_size |  |  |  | x |  |  |  |  |  |  |  |  |  |
Acu_notify_in_a_ext_parms |  |  |  |  |  |  |  |  |  |  |  |  |  |
Acu_notify_in_ext_parms_nb |  |  |  |  |  |  |  |  |  |  |  |  |  |
Acu_notify_in_ext_parms_lgth |  |  |  |  |  |  |  |  |  |  |  |  |  |
Acu_notify_in_a_q931, Acu_notify_in_q931_size |  |  | x |  | x |  |  |  |  |  |  | x |  | x

## ACU_NOTIFY_IN macro descriptions and Q.931 IE

Macro | Description | Q.931 IE
--- | --- | ---
Acu_notify_in_a_connected_name, Acu_notify_in_connected_name_size | Pointer to (and size of) buffer containing calling name. | Connected name
Acu_notify_in_a_ext_parms | Pointer to buffer containing extended parameters. | Not used.
Acu_notify_in_ext_parms_nb | Number of parameters in buffer containing extended parameters. | Not used.
Acu_notify_in_ext_parms_lgth | Total length of buffer containing extended parameters. | Not used.
Acu_notify_in_a_q931, Acu_notify_in_q931_size | Pointer to (and size of) buffer containing raw data of incoming Q.931 message. | Does not map to an IE.