# Hdlc[x].RxTimeSlot

Specifies the TDM timeslot of the receiving HDLC
channel for a specific trunk.

#### Syntax

Hdlc[x].RxTimeSlot = timeslot

x = 0-(n-1) (0-based trunk number or range of trunk numbers where n equals the number of trunks on the board.)

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0..31 (timeslot or range of timeslots)

#### Example

Hdlc[0..7].RxTimeSlot = 16

#### See also

Hdlc[x].Boot, Hdlc[x].TxTimeSlot