# dsx1SignalMode

Signal mode of the circuit.

#### Syntax

Integer

#### Access

Read/write

#### OID

p.6.1.11.n, where n = the index number of the DS1 interface.

#### Details

Valid entries include:

Type | Value | Description
--- | --- | ---
none | 1 | No bits are reserved for signaling on this channel.
robbedBit | 2 | T1 robbed bit signaling is in use.
bitOriented | 3 | E1 channel associated signaling is in use.
messageOriented | 4 | Common channel signaling is in use either on channel 16 of an E1 link or on channel 24 of a T1 link.