# Installation summary

The following table summarizes the procedure for installing the hardware and software components:

Step | Action
--- | ---
1 | Ensure that your host chassis meets the system requirements.
2 | Power down the system if it is running.
3 | If necessary, configure the CG 6060 board for H.100 bus termination.
4 | Install the CG 6060 board in a PCI bus slot.
5 | Power up the system.
6 | If NaturalAccess is not already installed, install Natural Access. This also installs the CG board driver and runtime software. The hardware interface drivers are installed with Natural Access software.
7 | For each board, create a board keyword file that details the board configuration settings. Find the closest example file in \nms\cg\cfg and use it as a baseline.
8 | Create a system configuration file that identifies all boards in the system and their associated board keyword files. For more information, refer to Configuring and starting the system with oamsys and the Dialogic® NaturalAccess™ OAM System Developer’s Manual.
9 | Configure an Ethernet connection. For more information, refer to either Configuring IPv4 Ethernet connections or Configuring IPv6 Ethernet connections.
10 | Run oamsys to configure the boards as specified in the configuration files.
11 | Connect the board interfaces to T1 or E1 trunks (if configured) and Ethernet connections.
12 | Verify that your installation is operational.