# ADI_FSKRECEIVE_PARMS

#### Dependent function: adiStartReceivingFSK

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
baudrate | DWORD | 1200 | integer | Transmission baud rate. 1200 is the only valid value.
droptime | DWORD | 5 | ms | Minimum dropout to silence before a packet is considered terminated.
minlevel | INT32 | -35 | dBm | Required minimum receive level.
minmark | DWORD | 10 | ms | Minimum required initial mark and seizure time.