# emckwAllowedRange

Range of allowed values for the EMC keyword.

#### Syntax

DisplayString (SIZE 0..255)

#### Access

Read-only

#### OID

p.3.1.1.7.n

#### Details

If the keyword type is integer, and is a yes or no choice, emckwAllowedRange contains a string in this format:

Nb values=2: Yes,No

If the keyword type is integer, and can take a range of values, emckwAllowedRange contains a string in this format:

BASE base:min_value <> max_value

where:

- base is a mathematical base of the integer (for example, 16 for a hexadecimal number).

- min_value is the minimum allowed value.

- max_value is the maximum allowed value.

For example:

BASE 10: 0 <> 65535

If the keyword type is string, emckwAllowedRange contains all the allowed strings for this keyword, separated by commas (,). For example: YES,NO. If any string is acceptable, this field contains <no range>.

emckwAllowedRange reflects the combined values of the Base, Min, Max, and Choices qualifiers for the keyword in the NMS OAM database.

#### Configuration

When it starts up, the OAM Database SNMP agent populates all MIB tables based upon information from the NMS OAM database. For more information, refer to OAM EMC table.