# snmpTrunkLog

Shows the status of digital trunks of each board in a chassis.

#### Usage

snmpTrunkLog address options

where:

Parameter | Description
--- | ---
address | Address or DNS name of a local or remote host running the SNMP agent about which to return information.

Valid options include:

Option | Description
--- | ---
-cc ommunity_name | Specify a community name. The default is public.
-rn | Number of retries. The default is 1 retry.
-tn | Timeout in hundredths of a second. The default is 100 (1 second).

snmpTrunkLog is similar to the trunkmon utility. See the NMS OAM System User's Manual for information.

#### Procedure

Complete the following steps to run snmpTrunkLog:

Step | Action
1 | From the command line, navigate to the \nms\ctaccess\demos\snmp\snmptrunklog directory (or the /opt/nms/ctaccess/demos/snmp/snmptruklog directory under UNIX).
2 | Enter the following command: snmpTrunkLog <address> where address is the IP address for the machine.

The following example shows how to run snmpTrunkLog:

> snmpTrunkLog
SNMP Demonstration and Test Program V.3.0 Nov 15 1999
NMS Communications Corporation.
Usage:
snmpChassScan [Address | DNSName] [options]
Address: default is 127.0.0.1
options: -cCommunity_name, specify community default is 'public'
-rN , retries default is N = 1 retry
-tN , timeout in hundredths-seconds default is N = 100 = 1 second
h Help S Sys info L Trunk list Q Quit
SEND A REQUEST FOR SYSTEM INFO TO: 10.1.20.45
System information:
System: Hardware: x86 Family 6 Model 3 Stepping 4 AT/AT COMPATIBLE - Software: Windows 2000
SysUpTime: 1:59:37.45
SysContact: Joe Kilroy
Computer name: KILROY
Location: NMS
SEND A REQUEST FOR TRUNKS TO: 10.1.20.45
Interface:2 Board:1 (AG_4040_1TE) Trunk:0 Status: Loss of frame, NoSgnl
Interface:3 Board:1 (AG_4040_1TE) Trunk:1 Status: Loss of frame, NoSgnl
Interface:4 Board:1 (AG_4040_1TE) Trunk:2 Status: Loss of frame, NoSgnl
Interface:5 Board:1 (AG_4040_1TE) Trunk:3 Status: Loss of frame, NoSgnl
Interface:6 Board:2 (AG_4040_2TE) Trunk:0 Status: In service
Interface:7 Board:2 (AG_4040_2TE) Trunk:1 Status: Loss of frame, NoSgnl
Interface:8 Board:2 (AG_4040_2TE) Trunk:2 Status: In service
Interface:9 Board:2 (AG_4040_2TE) Trunk:3 Status: Loss of frame, NoSgnl