# Hot Swap EMC keyword summary

The following table summarizes the Hot Swap EMC keywords that you can change. The Readonly qualifier for these keywords is set to No:

To... | Use this keyword...
--- | ---
Initiate insertion or extraction of a board | Board.boardname.Command

The following table summarizes the keywords that cannot be changed. The Readonly qualifier for these keywords is set to Yes:

To... | Use these keywords...
--- | ---
Determine the Hot Swap state of a board | Board.boardname.State
Retrieve information about the Hot Swap managed object | Name Version.Major Version.Minor

For more information, refer to the following topics:

To learn more about... | Refer to...
Using Hot Swap | Hot Swap board insertion and removal processes
Setting and retrieving keywords | Accessing configuration data
Specifying keywords in configuration files using NMS OAM utilities | NMS OAM System User's Manual
Setting and retrieving keywords from the command line | Keyword enumeration and setting: oaminfo