# General hardware specifications

This topic describes:

- Mechanical specifications

- H.110 compliant interface

- Host interface

- Environment

- Power requirements

## Mechanical specifications

The AG 2000C board has:

- 64K x 16 of SRAM

- A T8100A, which provides CT bus switching

- 4 MB of DRAM

- 100 MIPS C549 parts

- NS486SXL-25

TDM bus | Features one complete H.110 bus interface
DSP processing power | Four Texas Instruments TMS320VC549GGU-100 DSPs at 100 MIPS
Microprocessor | One 25 MHz 80486-compatible embedded processor
Board weight | Main board: .80 lb (.36 kg) Daughterboard: .05 lb (.02 kg) Rear transition board: .35 lb (.16 kg)
Software | Natural Access for Windows, UNIX, or Red Hat Linux

The AG 2000C board has indicators (LEDs) on the end bracket of the board as shown in Status indicator LEDs.

## H.110 compliant interface

- Flexible connectivity between line interfaces, DSPs, and H.110 bus.

- Switchable access to any of 4096 H.110 timeslots.

- H.110 clock master or clock slave (software-selectable).

- Compatible with any H.110-compliant telephony interface.

## Host interface

Feature | Specification
--- | ---
Electrical | CompactPCI bus designed to CompactPCI PICMG specification revision 2.1
Mechanical | Designed to the CompactPCI PICMG specification revision 2.1 for 6U style cards
Bus speed | 33 MHz, 32-bit master or slave
Memory | 128 K on-board interface memory

## Environment

Feature | Description
--- | ---
Operating temperature | 0 to 50 degrees C
Storage temperature | -20 to 70 degrees C
Humidity | 5% to 80%, non-condensing

## Power requirements

### AG 2000C-24

+12V @ 200 mA

-12V @ 250 mA

+5 V @ 1.5 A (400 MIPS)

+3.3 V @ 0.5 A