# Sample PPX configuration file

The following PPX configuration file contains sample switch definitions for a variety of NMS boards:

# ppx.cfg
#
# --- Point-to-Point Switching Service ---
# --- Configuration ---
#
# This file defines to the point-to-point switching service
# the available bus, timeslots, and switches it may use for
# establishing connection paths.
#
# This configuration file contains example switch definitions
# for various NMS boards. Use this as a guide for
# configuring the PPX service to your particular hardware
# configuration.
#
# Some Reminders:
# - All switch numbers must be unique.
# - The "DeviceNumber" is the logical board number established
# with OAM board configuration.
# - The PPX service speaks MVIP-95, not MVIP-90.
#
#
[PPX]
Fabric
IdleCode = MU_LAW # Default idle pattern [ MU_LAW | A_LAW ]
Bus H100 # H100 bus
CTBUS:0..15:0..31 # 2 mbps Clocking
CTBUS:16..23:0..63 # 4 mbps "
CTBUS:24..31:0..127 # 8 mbps "
End Bus
Switch 0 # CG 6000
SwitchType = HMIC
DeviceName = "agsw"
DeviceNumber = 0
Bus H100 ()
Inputs
LOCAL:0..14(2):0..23 # Trunk (0..29 for E1)
LOCAL:16..18(2):0..127 # DSP
End Inputs
Outputs
LOCAL:1..15(2):0..23 # Trunk (0..29 for E1)
LOCAL:17..19(2):0..127 # DSP
End Outputs
End Switch
# Switch 1 # CG 6100
# SwitchType = HMIC
# DeviceName = "agsw"
# DeviceNumber = 1
# Bus H100 ()
# Inputs
# LOCAL:0..62(2):0..29 # Trunk (0..23 for T1)
# LOCAL:64..66(2):0..479 # DSP
# End Inputs
# Outputs
# LOCAL:1..63(2):0..29 # Trunk (0..23 for T1)
# LOCAL:65..67(2):0..479 # DSP
# End Outputs
# End Switch
# Switch 2 # AG 4040
# SwitchType = HMIC
# DeviceName = "agsw"
# DeviceNumber = 2
# Bus H100 ()
# Inputs
# LOCAL:0..6(2):0..23 # Trunk
# LOCAL:16..18(2):0..127 # DSP
# End Inputs
# Outputs
# LOCAL:1..7(2):0..23 # Trunk
# LOCAL:17..19(2):0..127 # DSP
# End Outputs
# End Switch
# Switch 3 # AG 4040C
# SwitchType = HMIC
# DeviceName = "agsw"
# DeviceNumber = 3
# Bus H100 ()
# Inputs
# LOCAL:0..14(2):0..23 # Trunk (E1: 0..29)
# End Inuputs
# Outputs
# LOCAL:1..15(2):0..23 # Trunk (E1: 0..29)
# End Outputs
# End Switch
# Switch 4 # AG 2000
# SwitchType = HMIC
# DeviceName = "agsw"
# DeviceNumber = 4
# Bus H100 ()
# Inputs
# LOCAL:0..2(2):0..7 # Trunk
# LOCAL:4..6(2):0..7 # DSP
# End Inputs
# Outputs
# LOCAL:1..3(2):0..7 # Trunk
# LOCAL:5..7(2):0..7 # DSP
# End Outputs
# End Switch
# Switch 5 # AG 2000C
# SwitchType = HMIC
# DeviceName = "agsw"
# DeviceNumber = 5
# Bus H100 ()
# Inputs
# LOCAL:0..2(2):0..23 # Trunk
# LOCAL:4..6(2):0..23 # DSP
# End Inputs
# Outputs
# LOCAL:1..3(2):0..23 # Trunk
# LOCAL:5..7(2):0..23 # DSP
# End Outputs
# End Switch
# Switch 6 # QX 2000/100-4L
# SwitchType = HMIC
# DeviceName = "qxsw"
# DeviceNumber = 6
# Bus H100 ()
# Inputs
# LOCAL:0..6(2):0..3 # line interfaces & DSP resources
# LOCAL:8..10(2):0 # local phone data and signal
# LOCAL:12:0 # audio
# End Inputs
# Outputs
# LOCAL:1..7(2):0..3 # line interfaces & DSP resources
# LOCAL:9..11(2):0 # local phone data and signal
# LOCAL:13:0 # audio
# End Outputs
# End Switch
# Switch 7 # CX 2000C
# SwitchType = HMIC
# DeviceName = "cxsw"
# DeviceNumber = 7
# Bus H100 ()
# Inputs
# LOCAL:0..2(2):0..47 # 48 station interfaces
# LOCAL:4..6(2):0..47 # :0..31 for CX2000C-32
# End Inputs # :0..15 for CX2000C-16
# Outputs
# LOCAL:1..3(2):0..47 # 48 station interfaces
# LOCAL:5..7(2):0..47 # :0..31 for CX2000C-32
# End Outputs # :0..15 for CX2000C-16
# End Switch
# Connect
# 0:local:0:0 to 0:local:17:0 QUAD
# 0:local:0:2 to 0:local:17:2 QUAD NAILED
# End Connect
End Fabric