# ADI_ENERGY_PARMS

#### Dependent function: adiStartEnergyDetector

Field name | Type | Default | Units | Description
--- | --- | --- | --- | ---
autostop | DWORD | 1 | mask | Controls whether the energy detector continues running after the first event. Set this value to 1 to stop after the first event, or 0 to run continuously.
deglitch | DWORD | 20 | ms | Minimum time before a transition between silence and energy is recognized. Valid AG board and CG board range is 0 through 32767.
thresholdampl | INT32 | -45 | dBm | Minimum signal level that is considered to be energy. Anything below this level is considered to be silence. Valid AG board and CG board range is -51 through -15.