# Dialogic® MD1 RJ-21 male to MD1 RJ-21 cable

The shielded Dialogic® MD1 RJ-21 male to MD1 RJ-21 cable is available as a straight cable (P/N 83225) or with a right angle (P/N 83228). The following illustrations show these cables:

### P/N 83225:

### P/N 83228:

Caution: | The right angle connector does not comply with TIA-568 bend radius specifications (NEBS).

## Pin assignments

The pin assignments from P1 to P2 are 1:1. Twisted pairs are wired straight through, progressing as follows: 1 and 26, 2 and 27, 3 and 28, 4 and 29, and so forth, up to 25 and 50.