# NetworkInterface.Analog[x].ConfigFile

Specifies the country-specific file for AG 2000C loop start boards. Refer to QSLAC files and trunk control programs for more information.

#### Syntax

NetworkInterface.Analog[x].ConfigFile = filename

x = line number 0..23

#### Access

Read/Write

#### Type

Filename

#### Default

Filename | Where used
--- | ---
a2usals6.slc | Default. Loop start for 600 Ohm PBXs in North America and South America.
a2canls6.slc | Loop start for 600 Ohm PBXs in Canada.
a2jpnls6.slc | Loop start for 600 Ohm PBXs in Japan.
a2usals9.slc | Loop start for 900 Ohm PBXs in North America and South America.
a2canls9.slc | Loop start for 900 Ohm PBXs in Canada.
a2jpnls9.slc | Loop start for 900 Ohm PBXs in Japan.
a2usalsn.slc | PSTN connections in North America and South America.
a2canlsn.slc | PSTN connections in Canada.
a2jpnlsn.slc | PSTN connections in Japan.
a2eurlsc.slc | PSTN connections in the EU countries.
a2auslsc.slc | PSTN connections for Australia.

#### Allowed values

Valid QSLAC file name.

#### Example

NetworkInterface.Analog[0..23].ConfigFile = a2usals9.slc