# boardCommand

Turns the board on or off.

#### Syntax

Integer

#### Access

Read/write

#### OID

p.4.3.1.11.n, where n is the entry number.

#### Details

Setting the value of this object turns the board on or off. Check the boardStatus object to see when the command completes. Valid values:

Value | Action
--- | ---
1 | On (same as closing the handles in physical Hot Swap).
2 | Off (same as opening the handles in physical Hot Swap).

An operation must complete (not be in the pending state) before issuing a second command.

Note: The value of this object applies only to CompactPCI boards.